云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_80, M_80, L_80
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_80, M_80, L_80
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_80, M_80, L_80
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_80, M_80, L_80
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202508031236190000] 入待发送队列
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202508031236190001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202508031236190002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031236190000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
iot_status:0
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031236190002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031236190001,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202508031237200003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031237200003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202508031238210004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031238210004,提交成功(0)
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202508031239220005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031239220005,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202508031240230006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031240230006,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
data[type=4,serial=006EA1B2C3D4E5202508031241100007] 入待发送队列
push data[type=4, serial=MBCP00000008, len=457] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
运行状态数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031241100007,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202508031241240008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031241240008,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/9
data[type=512,serial=006EA1B2C3D4E5202508031242250009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031242250009,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/10
data[type=512,serial=006EA1B2C3D4E5202508031243260010] 入待发送队列
push data[type=512, serial=MBCP00000011, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031243260010,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/11
data[type=512,serial=006EA1B2C3D4E5202508031244270011] 入待发送队列
iot_status:0
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000012, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031244270011,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/12
data[type=512,serial=006EA1B2C3D4E5202508031245280012] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031245280012,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/13
data[type=512,serial=006EA1B2C3D4E5202508031246290013] 入待发送队列
push data[type=512, serial=MBCP00000014, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031246290013,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/14
data[type=512,serial=006EA1B2C3D4E5202508031247300014] 入待发送队列
push data[type=512, serial=MBCP00000015, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031247300014,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/15
data[type=512,serial=006EA1B2C3D4E5202508031248310015] 入待发送队列
push data[type=512, serial=MBCP00000016, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031248310015,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/16
data[type=512,serial=006EA1B2C3D4E5202508031249320016] 入待发送队列
push data[type=512, serial=MBCP00000017, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031249320016,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/17
data[type=512,serial=006EA1B2C3D4E5202508031250330017] 入待发送队列
push data[type=512, serial=MBCP00000018, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508031250330017,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
