云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=007D503250100410202507160903450000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：4_[Lc], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：5_[Lm], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[Lk], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：7_[Llk], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503250100410202507160904460001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503250100410202507160905470002] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：4_[Lc], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：5_[Lm], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[Lk], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：7_[Llk], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503250100410202507160906480003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=007D503250100410202507160907280004] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=007D503250100410202507160907280005] 入待发送队列
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=007D503250100410202507160918070000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：4_[Lc], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：5_[Lm], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[Lk], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：7_[Llk], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503250100410202507160919080001] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：4_[Lc], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：5_[Lm], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[Lk], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：7_[Llk], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_798, M_798, L_130164, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1197, M_1197, L_129366, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_798, M_798, L_130164, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_798, M_798, L_134568, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：4_[Lc], [PRINT]S_1197, M_1197, L_129366, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：5_[Lm], [PRINT]S_798, M_798, L_130164, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[Lk], [PRINT]S_798, M_798, L_131705, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：7_[Llk], [PRINT]S_798, M_798, L_130164, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=007D503250100410202507160919310003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=1, serial=MBCP00000001, len=1126] via MB SUCCESSED, 剩余:2
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_798, M_798, L_130164, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1197, M_1197, L_129366, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_798, M_798, L_130164, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_798, M_798, L_134568, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：4_[Lc], [PRINT]S_1197, M_1197, L_129366, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：5_[Lm], [PRINT]S_798, M_798, L_130164, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：6_[Lk], [PRINT]S_798, M_798, L_131705, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：7_[Llk], [PRINT]S_798, M_798, L_130164, [FLASH]S_0, M_1936800, L_0
HTTP丢包率：1/1
data[type=512,serial=007D503250100410202507160920090004] 入待发送队列
wait data[type=1, serial=007D503250100410202507160919310003] 响应超时(20), 丢弃
Total consumption of ink on startup：0_[K], [PRINT]S_1596, M_1596, L_260328, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_2394, M_2394, L_258732, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1596, M_1596, L_260328, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1596, M_1596, L_269142, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：4_[Lc], [PRINT]S_2394, M_2394, L_258732, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：5_[Lm], [PRINT]S_1596, M_1596, L_260328, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：6_[Lk], [PRINT]S_1596, M_1596, L_263410, [FLASH]S_0, M_1936800, L_0
Total consumption of ink on startup：7_[Llk], [PRINT]S_1596, M_1596, L_260328, [FLASH]S_0, M_1936800, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=007D503250100410202507160920150005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000002, len=1126] via MB SUCCESSED, 剩余:2
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=2, serial=007D503250100410202507160920150005] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160921100006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160922110007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160923120008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160924130009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160925140010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160926150011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160927160012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160928170013] 入待发送队列
data[type=4,serial=007D503250100410202507160928380014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160929180015] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160930190016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160931200017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160932210018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160933220019] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=007D503250100410202507160933380020] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160934230021] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160942250022] 入待发送队列
data[type=4,serial=007D503250100410202507160942250023] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160943260024] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160944270025] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503250100410202507160945280026] 入待发送队列
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507160959170000] 入待发送队列
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_760, M_760, L_760
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
iot_ccid:CCID-123, imei:IMEI-123
data[type=256,serial=006EA1B2C3D4E5202507160959170001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507160959170002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507160959170000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507160959170002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507160959170001,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
iot_status:0
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507161913250000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_140, M_140, L_140
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_140, M_140, L_140
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_140, M_140, L_140
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_140, M_140, L_140
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_240, M_240, L_240
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507161913250001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507161913250002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507161913250000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507161913250002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507161913250001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507161914260003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507161914260003,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202507161915270004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507161915270004,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202507161916280005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507161916280005,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202507161917290006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507161917290006,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
