云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311718300000] 入待发送队列
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311719310001] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311720320002] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311721330003] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311722340004] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500102202507311722530005] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311723350006] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311724360007] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311725370008] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311726380009] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311727390010] 入待发送队列
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500102202507311727530011] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311728400012] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311729410013] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311730420014] 入待发送队列
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311752090015] 入待发送队列
data[type=4,serial=00F4503250500102202507311752120016] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311753100017] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311754110018] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311755120019] 入待发送队列
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311756130020] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500102202507311757120021] 入待发送队列
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311757140022] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311758150023] 入待发送队列
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:9.997227-9.997227-19.994453
data[type=2,serial=00F4503250500102202507311758270024] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311759160025] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311800170026] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311801180027] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500102202507311802120028] 入待发送队列
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311802190029] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311803200030] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311804210031] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311805220032] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311806230033] 入待发送队列
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500102202507311807120034] 入待发送队列
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311807240035] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311808250036] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311809260037] 入待发送队列
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311811090000] 入待发送队列
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311812100001] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311813110002] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311814120003] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311815130004] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500102202507311815540005] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311816140006] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311817150007] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311818160008] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311819170009] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311820180010] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311821190011] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311822200012] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311823210013] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311824220014] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311825230015] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311826240016] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311827250017] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311828260018] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311829270019] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311830280020] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311831290021] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311832300022] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311833310023] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311836430024] 入待发送队列
data[type=4,serial=00F4503250500102202507311836460025] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311837440026] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311838450027] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311839460028] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311840470029] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311841480030] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311842490031] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311843500032] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311844510033] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311845520034] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311846530035] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311847540036] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311848550037] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311849560038] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311850570039] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311851580040] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311852590041] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311854000042] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311855010043] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311856020044] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311857030045] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311858040046] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311859050047] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311900060048] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311901070049] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311902080050] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311903090051] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311904100052] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311905110053] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311906120054] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311907130055] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311908140056] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311909150057] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311910160058] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311911170059] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311912180060] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311913190061] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311914200062] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311915210063] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311916220064] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311917230065] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311918240066] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311919250067] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311920260068] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311921270069] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311922280070] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311923290071] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311924300072] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311925310073] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311926320074] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311927330075] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311928340076] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311929350077] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311930360078] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311931370079] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500102202507311932380080] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_320, M_320, L_320
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507312058460000] 入待发送队列
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507312058460001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507312058460002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312058460000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
iot_status:0
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312058460002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312058460001,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507312059470003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312059470003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202507312100480004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312100480004,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202507312101490005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312101490005,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202507312102500006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312102500006,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
data[type=4,serial=006EA1B2C3D4E5202507312103370007] 入待发送队列
push data[type=4, serial=MBCP00000008, len=419] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
运行状态数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312103370007,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202507312103510008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312103510008,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/9
data[type=512,serial=006EA1B2C3D4E5202507312104520009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312104520009,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/10
data[type=512,serial=006EA1B2C3D4E5202507312204330010] 入待发送队列
push data[type=512, serial=MBCP00000011, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
iot_ccid:CCID-123, imei:IMEI-123
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312204330010,提交成功(0)
HTTP丢包率：0/11
data[type=512,serial=006EA1B2C3D4E5202507312216480011] 入待发送队列
push data[type=512, serial=MBCP00000012, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312216480011,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/12
data[type=512,serial=006EA1B2C3D4E5202507312217490012] 入待发送队列
push data[type=512, serial=MBCP00000013, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312217490012,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/13
data[type=512,serial=006EA1B2C3D4E5202507312218500013] 入待发送队列
push data[type=512, serial=MBCP00000014, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312218500013,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/14
data[type=512,serial=006EA1B2C3D4E5202507312219510014] 入待发送队列
push data[type=512, serial=MBCP00000015, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312219510014,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/15
data[type=512,serial=006EA1B2C3D4E5202507312220520015] 入待发送队列
push data[type=512, serial=MBCP00000016, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312220520015,提交成功(0)
iot_status:0
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/16
data[type=512,serial=006EA1B2C3D4E5202507312221530016] 入待发送队列
push data[type=512, serial=MBCP00000017, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312221530016,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/17
data[type=512,serial=006EA1B2C3D4E5202507312222540017] 入待发送队列
push data[type=512, serial=MBCP00000018, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312222540017,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/18
data[type=512,serial=006EA1B2C3D4E5202507312223550018] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000019, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312223550018,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/19
data[type=512,serial=006EA1B2C3D4E5202507312224560019] 入待发送队列
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000020, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312224560019,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/20
data[type=512,serial=006EA1B2C3D4E5202507312225570020] 入待发送队列
push data[type=512, serial=MBCP00000021, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312225570020,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/21
data[type=512,serial=006EA1B2C3D4E5202507312226580021] 入待发送队列
push data[type=512, serial=MBCP00000022, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312226580021,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/22
data[type=512,serial=006EA1B2C3D4E5202507312227590022] 入待发送队列
push data[type=512, serial=MBCP00000023, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312227590022,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/23
data[type=512,serial=006EA1B2C3D4E5202507312229000023] 入待发送队列
push data[type=512, serial=MBCP00000024, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312229000023,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/24
data[type=512,serial=006EA1B2C3D4E5202507312230010024] 入待发送队列
push data[type=512, serial=MBCP00000025, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312230010024,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/25
data[type=512,serial=006EA1B2C3D4E5202507312231020025] 入待发送队列
push data[type=512, serial=MBCP00000026, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312231020025,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/26
data[type=512,serial=006EA1B2C3D4E5202507312232030026] 入待发送队列
push data[type=512, serial=MBCP00000027, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312232030026,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/27
data[type=512,serial=006EA1B2C3D4E5202507312233040027] 入待发送队列
push data[type=512, serial=MBCP00000028, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312233040027,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/28
data[type=512,serial=006EA1B2C3D4E5202507312234050028] 入待发送队列
push data[type=512, serial=MBCP00000029, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312234050028,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_880, M_880, L_880
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_880, M_880, L_880
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_880, M_880, L_880
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_880, M_880, L_880
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/29
data[type=512,serial=006EA1B2C3D4E5202507312235060029] 入待发送队列
push data[type=512, serial=MBCP00000030, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312235060029,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/30
data[type=512,serial=006EA1B2C3D4E5202507312236070030] 入待发送队列
push data[type=512, serial=MBCP00000031, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312236070030,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/31
data[type=512,serial=006EA1B2C3D4E5202507312256560031] 入待发送队列
push data[type=512, serial=MBCP00000032, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312256560031,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/32
data[type=512,serial=006EA1B2C3D4E5202507312300160032] 入待发送队列
push data[type=512, serial=MBCP00000033, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312300160032,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/33
data[type=512,serial=006EA1B2C3D4E5202507312301170033] 入待发送队列
push data[type=512, serial=MBCP00000034, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312301170033,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/34
data[type=512,serial=006EA1B2C3D4E5202507312302180034] 入待发送队列
push data[type=512, serial=MBCP00000035, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507312302180034,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
