云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
CloudServiceCore线程退出
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041519370000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_30240, M_23719, L_242729, [FLASH]S_0, M_0, L_4948800
Total consumption of ink on startup：1_[C], [PRINT]S_29360, M_23920, L_237528, [FLASH]S_0, M_0, L_4948800
Total consumption of ink on startup：2_[M], [PRINT]S_29616, M_23664, L_237528, [FLASH]S_0, M_0, L_4948800
Total consumption of ink on startup：3_[Y], [PRINT]S_29040, M_24240, L_237528, [FLASH]S_0, M_0, L_4948800
Total consumption of ink on startup：8_[W], [PRINT]S_58520, M_48352, L_477470, [FLASH]S_0, M_0, L_9894400
Total consumption of ink on startup：9_[V], [PRINT]S_29612, M_23824, L_242087, [FLASH]S_0, M_0, L_4950400
Total consumption of ink on startup：10_[V1], [PRINT]S_29292, M_24144, L_238609, [FLASH]S_0, M_0, L_4950400
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041520380001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041521390002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=392] via MB SUCCESSED, 剩余:0
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041522400003] 入待发送队列
iot_status:3
iot_status:0
iot_status:3
iot_status:0
wait data[type=512, serial=007D503240501609202508041521390002] 响应超时(20), 丢弃
push data[type=512, serial=MBCP00000002, len=392] via MB SUCCESSED, 剩余:0
Total consumption of ink on startup：0_[K], [PRINT]S_30240, M_23719, L_242729, [FLASH]S_0, M_0, L_9812800
Total consumption of ink on startup：1_[C], [PRINT]S_29360, M_23920, L_237528, [FLASH]S_0, M_0, L_9812800
Total consumption of ink on startup：2_[M], [PRINT]S_29616, M_23664, L_237528, [FLASH]S_0, M_0, L_9812800
Total consumption of ink on startup：3_[Y], [PRINT]S_29040, M_24240, L_237528, [FLASH]S_0, M_0, L_9812800
Total consumption of ink on startup：8_[W], [PRINT]S_58520, M_48352, L_477470, [FLASH]S_0, M_0, L_19622400
Total consumption of ink on startup：9_[V], [PRINT]S_29612, M_23824, L_242087, [FLASH]S_0, M_0, L_9814400
Total consumption of ink on startup：10_[V1], [PRINT]S_29292, M_24144, L_238609, [FLASH]S_0, M_0, L_9814400
Total consumption of ink on startup：0_[K], [PRINT]S_60448, M_47415, L_484964, [FLASH]S_0, M_0, L_9812800
Total consumption of ink on startup：1_[C], [PRINT]S_58720, M_47840, L_475056, [FLASH]S_0, M_0, L_9812800
Total consumption of ink on startup：2_[M], [PRINT]S_59232, M_47328, L_475056, [FLASH]S_0, M_0, L_9812800
Total consumption of ink on startup：3_[Y], [PRINT]S_58080, M_48480, L_475056, [FLASH]S_0, M_0, L_9812800
Total consumption of ink on startup：8_[W], [PRINT]S_117040, M_96704, L_954940, [FLASH]S_0, M_0, L_19622400
Total consumption of ink on startup：9_[V], [PRINT]S_59224, M_47648, L_484383, [FLASH]S_0, M_0, L_9814400
Total consumption of ink on startup：10_[V1], [PRINT]S_58584, M_48288, L_477218, [FLASH]S_0, M_0, L_9814400
墨点大小,SMB:3.500000-6.000000-8.000000
data[type=2,serial=007D503240501609202508041523150004] 入待发送队列
iot_status:3
wait data[type=512, serial=007D503240501609202508041522400003] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508041523410005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508041524420006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000003, len=392] via MB SUCCESSED, 剩余:1
iot_status:3
iot_status:3
iot_status:3
iot_status:0
wait data[type=512, serial=007D503240501609202508041524420006] 响应超时(20), 丢弃
push data[type=2, serial=MBCP00000004, len=1113] via MB SUCCESSED, 剩余:0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_60448, M_47415, L_484964, [FLASH]S_0, M_0, L_14676800
Total consumption of ink on startup：1_[C], [PRINT]S_58720, M_47840, L_475056, [FLASH]S_0, M_0, L_14676800
Total consumption of ink on startup：2_[M], [PRINT]S_59232, M_47328, L_475056, [FLASH]S_0, M_0, L_14676800
Total consumption of ink on startup：3_[Y], [PRINT]S_58080, M_48480, L_475056, [FLASH]S_0, M_0, L_14676800
Total consumption of ink on startup：8_[W], [PRINT]S_117040, M_96704, L_954940, [FLASH]S_0, M_0, L_29350400
Total consumption of ink on startup：9_[V], [PRINT]S_59224, M_47648, L_484383, [FLASH]S_0, M_0, L_14678400
Total consumption of ink on startup：10_[V1], [PRINT]S_58584, M_48288, L_477218, [FLASH]S_0, M_0, L_14678400
HTTP丢包率：4/4
data[type=512,serial=007D503240501609202508041525430007] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_90656, M_71111, L_727199, [FLASH]S_0, M_0, L_14676800
Total consumption of ink on startup：1_[C], [PRINT]S_88080, M_71760, L_712584, [FLASH]S_0, M_0, L_14676800
Total consumption of ink on startup：2_[M], [PRINT]S_88848, M_70992, L_712584, [FLASH]S_0, M_0, L_14676800
Total consumption of ink on startup：3_[Y], [PRINT]S_87120, M_72720, L_712584, [FLASH]S_0, M_0, L_14676800
Total consumption of ink on startup：8_[W], [PRINT]S_175560, M_145056, L_1432410, [FLASH]S_0, M_0, L_29350400
Total consumption of ink on startup：9_[V], [PRINT]S_88836, M_71472, L_726609, [FLASH]S_0, M_0, L_14678400
Total consumption of ink on startup：10_[V1], [PRINT]S_87876, M_72432, L_715827, [FLASH]S_0, M_0, L_14678400
墨点大小,SMB:3.500000-6.000000-8.000000
data[type=2,serial=007D503240501609202508041525510008] 入待发送队列
iot_status:0
wait data[type=2, serial=007D503240501609202508041523150004] 响应超时(20), 重入待发送队列
push data[type=2, serial=MBCP00000005, len=1113] via MB SUCCESSED, 剩余:2
iot_status:3
iot_status:3
iot_status:3
wait data[type=2, serial=007D503240501609202508041523150004] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=007D503240501609202508041526440009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=007D503240501609202508041527450010] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000006, len=392] via MB SUCCESSED, 剩余:2
iot_status:3
iot_status:0
iot_status:3
iot_status:0
wait data[type=512, serial=007D503240501609202508041527450010] 响应超时(20), 丢弃
push data[type=2, serial=MBCP00000007, len=1113] via MB SUCCESSED, 剩余:1
iot_status:3
iot_status:0
iot_status:3
iot_status:3
wait data[type=2, serial=007D503240501609202508041523150004] 响应超时(20), 重入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_90656, M_71111, L_727199, [FLASH]S_0, M_0, L_19540800
Total consumption of ink on startup：1_[C], [PRINT]S_88080, M_71760, L_712584, [FLASH]S_0, M_0, L_19540800
Total consumption of ink on startup：2_[M], [PRINT]S_88848, M_70992, L_712584, [FLASH]S_0, M_0, L_19540800
Total consumption of ink on startup：3_[Y], [PRINT]S_87120, M_72720, L_712584, [FLASH]S_0, M_0, L_19540800
Total consumption of ink on startup：8_[W], [PRINT]S_175560, M_145056, L_1432410, [FLASH]S_0, M_0, L_39078400
Total consumption of ink on startup：9_[V], [PRINT]S_88836, M_71472, L_726609, [FLASH]S_0, M_0, L_19542400
Total consumption of ink on startup：10_[V1], [PRINT]S_87876, M_72432, L_715827, [FLASH]S_0, M_0, L_19542400
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041528460011] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_120864, M_94807, L_969434, [FLASH]S_0, M_0, L_19540800
Total consumption of ink on startup：1_[C], [PRINT]S_117440, M_95680, L_950112, [FLASH]S_0, M_0, L_19540800
Total consumption of ink on startup：2_[M], [PRINT]S_118464, M_94656, L_950112, [FLASH]S_0, M_0, L_19540800
Total consumption of ink on startup：3_[Y], [PRINT]S_116160, M_96960, L_950112, [FLASH]S_0, M_0, L_19540800
Total consumption of ink on startup：8_[W], [PRINT]S_234080, M_193408, L_1909880, [FLASH]S_0, M_0, L_39078400
Total consumption of ink on startup：9_[V], [PRINT]S_118448, M_95296, L_968909, [FLASH]S_0, M_0, L_19542400
Total consumption of ink on startup：10_[V1], [PRINT]S_117168, M_96576, L_954436, [FLASH]S_0, M_0, L_19542400
墨点大小,SMB:3.500000-6.000000-8.000000
data[type=2,serial=007D503240501609202508041528510012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041529470013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041530480014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=007D503240501609202508041531360015] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041537550016] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041538560017] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041539570018] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041540580019] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041541590020] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041543000021] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041544010022] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041545020023] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041546030024] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041547040025] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041548050026] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041549060027] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041550070028] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041551080029] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041552090030] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041553100031] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041554110032] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041555120033] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041556130034] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041557140035] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041558150036] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041559160037] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041600170038] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041601180039] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041602190040] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041603200041] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041604210042] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041623210043] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041624220044] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041625230045] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041626240046] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041627250047] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041628260048] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041629270049] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041630280050] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041631290051] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041632300052] 入待发送队列
HTTP丢包率：7/7
data[type=512,serial=007D503240501609202508041634010053] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[V], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V1], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041639050000] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041640060001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041641070002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041642080003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041643090004] 入待发送队列
data[type=4,serial=007D503240501609202508041643110005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041644100006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041645110007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041646120008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041647130009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041648140010] 入待发送队列
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:0
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041703410000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_2109251, M_1708416, L_72, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：1_[C], [PRINT]S_2112761, M_1702210, L_74, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：2_[M], [PRINT]S_2103163, M_1711748, L_43, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：3_[Y], [PRINT]S_2098436, M_1716507, L_72, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：8_[W], [PRINT]S_793479264, M_105612335, L_21147672, [FLASH]S_0, M_0, L_29184000
Total consumption of ink on startup：9_[V], [PRINT]S_3314, M_839, L_0, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：10_[V1], [PRINT]S_3679, M_84, L_0, [FLASH]S_0, M_0, L_14592000
push data[type=512, serial=MBCP00000001, len=392] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=007D503240501609202508041703410000] 响应超时(20), 丢弃
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
iot_status:3
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041706200000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_2109251, M_1708416, L_72, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：1_[C], [PRINT]S_2112761, M_1702210, L_74, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：2_[M], [PRINT]S_2103163, M_1711748, L_43, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：3_[Y], [PRINT]S_2098436, M_1716507, L_72, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：8_[W], [PRINT]S_793479264, M_105612335, L_21147672, [FLASH]S_0, M_0, L_29184000
Total consumption of ink on startup：9_[V], [PRINT]S_3314, M_839, L_0, [FLASH]S_0, M_0, L_14592000
Total consumption of ink on startup：10_[V1], [PRINT]S_3679, M_84, L_0, [FLASH]S_0, M_0, L_14592000
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_2109251, M_1708416, L_72, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：1_[C], [PRINT]S_2112761, M_1702210, L_74, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：2_[M], [PRINT]S_2103163, M_1711748, L_43, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：3_[Y], [PRINT]S_2098436, M_1716507, L_72, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：8_[W], [PRINT]S_793479264, M_105612335, L_21147672, [FLASH]S_0, M_0, L_39136000
Total consumption of ink on startup：9_[V], [PRINT]S_3314, M_839, L_0, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：10_[V1], [PRINT]S_3679, M_84, L_0, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：0_[K], [PRINT]S_2109251, M_1708416, L_72, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：1_[C], [PRINT]S_2112761, M_1702210, L_74, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：2_[M], [PRINT]S_2103163, M_1711748, L_43, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：3_[Y], [PRINT]S_2098436, M_1716507, L_72, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：8_[W], [PRINT]S_793479264, M_105612335, L_21147672, [FLASH]S_0, M_0, L_39136000
Total consumption of ink on startup：9_[V], [PRINT]S_3314, M_839, L_0, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：10_[V1], [PRINT]S_3679, M_84, L_0, [FLASH]S_0, M_0, L_19568000
iot_status:3
墨点大小,SMB:3.500000-6.000000-8.000000
data[type=2,serial=007D503240501609202508041707090001] 入待发送队列
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041707210002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041708220003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
iot_status:3
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041709190000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_2109251, M_1708416, L_72, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：1_[C], [PRINT]S_2112761, M_1702210, L_74, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：2_[M], [PRINT]S_2103163, M_1711748, L_43, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：3_[Y], [PRINT]S_2098436, M_1716507, L_72, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：8_[W], [PRINT]S_793479264, M_105612335, L_21147672, [FLASH]S_0, M_0, L_39136000
Total consumption of ink on startup：9_[V], [PRINT]S_3314, M_839, L_0, [FLASH]S_0, M_0, L_19568000
Total consumption of ink on startup：10_[V1], [PRINT]S_3679, M_84, L_0, [FLASH]S_0, M_0, L_19568000
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041710200001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041711210002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041712220003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041713230004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041714240005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041715250006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041716260007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041717270008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041718280009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041719290010] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_2109251, M_1708416, L_72, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：1_[C], [PRINT]S_2112761, M_1702210, L_74, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：2_[M], [PRINT]S_2103163, M_1711748, L_43, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：3_[Y], [PRINT]S_2098436, M_1716507, L_72, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：8_[W], [PRINT]S_793479264, M_105612335, L_21147672, [FLASH]S_0, M_0, L_49088000
Total consumption of ink on startup：9_[V], [PRINT]S_3314, M_839, L_0, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：10_[V1], [PRINT]S_3679, M_84, L_0, [FLASH]S_0, M_0, L_24544000
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_2660867, M_2155200, L_72, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：1_[C], [PRINT]S_2665625, M_2147746, L_74, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：2_[M], [PRINT]S_2653531, M_2159780, L_43, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：3_[Y], [PRINT]S_2647556, M_2165787, L_72, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：8_[W], [PRINT]S_815397752, M_106500911, L_21147672, [FLASH]S_0, M_0, L_49088000
Total consumption of ink on startup：9_[V], [PRINT]S_3314, M_839, L_0, [FLASH]S_0, M_0, L_24544000
Total consumption of ink on startup：10_[V1], [PRINT]S_3679, M_84, L_0, [FLASH]S_0, M_0, L_24544000
iot_status:0
墨点大小,SMB:3.500000-6.000000-8.000000
data[type=2,serial=007D503240501609202508041720280011] 入待发送队列
push data[type=2, serial=MBCP00000001, len=1005] via MB SUCCESSED, 剩余:1
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041720300012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
wait data[type=2, serial=007D503240501609202508041720280011] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=007D503240501609202508041721100013] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041729390014] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041730400015] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041731410016] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041732420017] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041733430018] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041734440019] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041735450020] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041736460021] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041737470022] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041738480023] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041739490024] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041741370025] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041742380026] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508041743390027] 入待发送队列
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202508041932590000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_20, M_20, L_20
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_20, M_20, L_20
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_20, M_20, L_20
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_20, M_20, L_20
Total consumption of ink on startup：4_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_240, M_240, L_240
Total consumption of ink on startup：5_[V], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
Total consumption of ink on startup：10_[T], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202508041933000001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202508041933000002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041932590000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041933000002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041933000001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202508041934000003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041934000003,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202508041935010004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041935010004,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202508041936020005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041936020005,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202508041937030006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041937030006,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
data[type=4,serial=006EA1B2C3D4E5202508041937470007] 入待发送队列
push data[type=4, serial=MBCP00000008, len=419] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
运行状态数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041937470007,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202508041938040008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041938040008,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/9
data[type=512,serial=006EA1B2C3D4E5202508041939050009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041939050009,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/10
data[type=512,serial=006EA1B2C3D4E5202508041940060010] 入待发送队列
push data[type=512, serial=MBCP00000011, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041940060010,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/11
data[type=512,serial=006EA1B2C3D4E5202508041941070011] 入待发送队列
push data[type=512, serial=MBCP00000012, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041941070011,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/12
data[type=512,serial=006EA1B2C3D4E5202508041942080012] 入待发送队列
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000013, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041942080012,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/13
data[type=512,serial=006EA1B2C3D4E5202508041943090013] 入待发送队列
push data[type=512, serial=MBCP00000014, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041943090013,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/14
data[type=512,serial=006EA1B2C3D4E5202508041944100014] 入待发送队列
push data[type=512, serial=MBCP00000015, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041944100014,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/15
data[type=512,serial=006EA1B2C3D4E5202508041945110015] 入待发送队列
push data[type=512, serial=MBCP00000016, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041945110015,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/16
data[type=512,serial=006EA1B2C3D4E5202508041946120016] 入待发送队列
push data[type=512, serial=MBCP00000017, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041946120016,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/17
data[type=512,serial=006EA1B2C3D4E5202508041952120017] 入待发送队列
push data[type=512, serial=MBCP00000018, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041952120017,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/18
data[type=512,serial=006EA1B2C3D4E5202508041954450018] 入待发送队列
iot_status:0
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000019, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041954450018,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/19
data[type=512,serial=006EA1B2C3D4E5202508041955460019] 入待发送队列
push data[type=512, serial=MBCP00000020, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041955460019,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/20
data[type=512,serial=006EA1B2C3D4E5202508041956470020] 入待发送队列
push data[type=512, serial=MBCP00000021, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041956470020,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/21
data[type=512,serial=006EA1B2C3D4E5202508041957480021] 入待发送队列
push data[type=512, serial=MBCP00000022, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202508041957480021,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041958580000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_556304597, M_984169190, L_980169582, [FLASH]S_0, M_0, L_92422400
Total consumption of ink on startup：1_[C], [PRINT]S_1987931168, M_892399029, L_385363443, [FLASH]S_0, M_0, L_92422400
Total consumption of ink on startup：2_[M], [PRINT]S_1047763295, M_751893324, L_1611069411, [FLASH]S_0, M_0, L_92422400
Total consumption of ink on startup：3_[Y], [PRINT]S_1252548035, M_94450973, L_2490664432, [FLASH]S_0, M_0, L_92422400
Total consumption of ink on startup：8_[W], [PRINT]S_16542440997, M_15385383, L_4299781, [FLASH]S_0, M_0, L_184838400
Total consumption of ink on startup：9_[V], [PRINT]S_308791, M_214416, L_2180207, [FLASH]S_0, M_0, L_92425600
Total consumption of ink on startup：10_[V1], [PRINT]S_285043, M_220022, L_2149875, [FLASH]S_0, M_0, L_92425600
Total consumption of ink on startup：0_[K], [PRINT]S_556304597, M_984169190, L_980169582, [FLASH]S_0, M_0, L_92422400
Total consumption of ink on startup：1_[C], [PRINT]S_1987931168, M_892399029, L_385363443, [FLASH]S_0, M_0, L_92422400
Total consumption of ink on startup：2_[M], [PRINT]S_1047763295, M_751893324, L_1611069411, [FLASH]S_0, M_0, L_92422400
Total consumption of ink on startup：3_[Y], [PRINT]S_1252548035, M_94450973, L_2490664432, [FLASH]S_0, M_0, L_92422400
Total consumption of ink on startup：8_[W], [PRINT]S_16542440997, M_15385383, L_4299781, [FLASH]S_0, M_0, L_184838400
Total consumption of ink on startup：9_[V], [PRINT]S_308791, M_214416, L_2180207, [FLASH]S_0, M_0, L_92425600
Total consumption of ink on startup：10_[V1], [PRINT]S_285043, M_220022, L_2149875, [FLASH]S_0, M_0, L_92425600
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508041959590001] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_556304597, M_984169190, L_980169582, [FLASH]S_0, M_0, L_97286400
Total consumption of ink on startup：1_[C], [PRINT]S_1987931168, M_892399029, L_385363443, [FLASH]S_0, M_0, L_97286400
Total consumption of ink on startup：2_[M], [PRINT]S_1047763295, M_751893324, L_1611069411, [FLASH]S_0, M_0, L_97286400
Total consumption of ink on startup：3_[Y], [PRINT]S_1252548035, M_94450973, L_2490664432, [FLASH]S_0, M_0, L_97286400
Total consumption of ink on startup：8_[W], [PRINT]S_16542440997, M_15385383, L_4299781, [FLASH]S_0, M_0, L_194566400
Total consumption of ink on startup：9_[V], [PRINT]S_308791, M_214416, L_2180207, [FLASH]S_0, M_0, L_97289600
Total consumption of ink on startup：10_[V1], [PRINT]S_285043, M_220022, L_2149875, [FLASH]S_0, M_0, L_97289600
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_556334805, M_984192886, L_980411817, [FLASH]S_0, M_0, L_97286400
Total consumption of ink on startup：1_[C], [PRINT]S_1987960528, M_892422949, L_385600971, [FLASH]S_0, M_0, L_97286400
Total consumption of ink on startup：2_[M], [PRINT]S_1047792911, M_751916988, L_1611306939, [FLASH]S_0, M_0, L_97286400
Total consumption of ink on startup：3_[Y], [PRINT]S_1252577075, M_94475213, L_2490901960, [FLASH]S_0, M_0, L_97286400
Total consumption of ink on startup：8_[W], [PRINT]S_16542499517, M_15433735, L_4777251, [FLASH]S_0, M_0, L_194566400
Total consumption of ink on startup：9_[V], [PRINT]S_338403, M_238240, L_2422522, [FLASH]S_0, M_0, L_97289600
Total consumption of ink on startup：10_[V1], [PRINT]S_314335, M_244166, L_2388484, [FLASH]S_0, M_0, L_97289600
墨点大小,SMB:3.500000-6.000000-8.000000
data[type=2,serial=007D503240501609202508042000220002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508042001000003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508042002010004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508042003020005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508042004030006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508042005040007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=007D503240501609202508042006050008] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=392] via MB SUCCESSED, 剩余:1
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=007D503240501609202508042006050008] 响应超时(20), 丢弃
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042007060009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042008070010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042009080011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_556334805, M_984192886, L_980411817, [FLASH]S_0, M_0, L_102153600
Total consumption of ink on startup：1_[C], [PRINT]S_1987960528, M_892422949, L_385600971, [FLASH]S_0, M_0, L_102153600
Total consumption of ink on startup：2_[M], [PRINT]S_1047792911, M_751916988, L_1611306939, [FLASH]S_0, M_0, L_102153600
Total consumption of ink on startup：3_[Y], [PRINT]S_1252577075, M_94475213, L_2490901960, [FLASH]S_0, M_0, L_102153600
Total consumption of ink on startup：8_[W], [PRINT]S_16542499517, M_15433735, L_4777251, [FLASH]S_0, M_0, L_204300800
Total consumption of ink on startup：9_[V], [PRINT]S_338403, M_238240, L_2422522, [FLASH]S_0, M_0, L_102156800
Total consumption of ink on startup：10_[V1], [PRINT]S_314335, M_244166, L_2388484, [FLASH]S_0, M_0, L_102156800
Total consumption of ink on startup：0_[K], [PRINT]S_556365013, M_984216582, L_980654052, [FLASH]S_0, M_0, L_102153600
Total consumption of ink on startup：1_[C], [PRINT]S_1987989888, M_892446869, L_385838499, [FLASH]S_0, M_0, L_102153600
Total consumption of ink on startup：2_[M], [PRINT]S_1047822527, M_751940652, L_1611544467, [FLASH]S_0, M_0, L_102153600
Total consumption of ink on startup：3_[Y], [PRINT]S_1252606115, M_94499453, L_2491139488, [FLASH]S_0, M_0, L_102153600
Total consumption of ink on startup：8_[W], [PRINT]S_16542558037, M_15482087, L_5254721, [FLASH]S_0, M_0, L_204300800
Total consumption of ink on startup：9_[V], [PRINT]S_368015, M_262064, L_2664812, [FLASH]S_0, M_0, L_102156800
Total consumption of ink on startup：10_[V1], [PRINT]S_343627, M_268310, L_2627093, [FLASH]S_0, M_0, L_102156800
墨点大小,SMB:3.500000-6.000000-8.000000
data[type=2,serial=007D503240501609202508042009580012] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042010090013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_556365013, M_984216582, L_980654052, [FLASH]S_0, M_0, L_107017600
Total consumption of ink on startup：1_[C], [PRINT]S_1987989888, M_892446869, L_385838499, [FLASH]S_0, M_0, L_107017600
Total consumption of ink on startup：2_[M], [PRINT]S_1047822527, M_751940652, L_1611544467, [FLASH]S_0, M_0, L_107017600
Total consumption of ink on startup：3_[Y], [PRINT]S_1252606115, M_94499453, L_2491139488, [FLASH]S_0, M_0, L_107017600
Total consumption of ink on startup：8_[W], [PRINT]S_16542558037, M_15482087, L_5254721, [FLASH]S_0, M_0, L_214028800
Total consumption of ink on startup：9_[V], [PRINT]S_368015, M_262064, L_2664812, [FLASH]S_0, M_0, L_107020800
Total consumption of ink on startup：10_[V1], [PRINT]S_343627, M_268310, L_2627093, [FLASH]S_0, M_0, L_107020800
Total consumption of ink on startup：0_[K], [PRINT]S_556395221, M_984240278, L_980896287, [FLASH]S_0, M_0, L_107017600
Total consumption of ink on startup：1_[C], [PRINT]S_1988019248, M_892470789, L_386076027, [FLASH]S_0, M_0, L_107017600
Total consumption of ink on startup：2_[M], [PRINT]S_1047852143, M_751964316, L_1611781995, [FLASH]S_0, M_0, L_107017600
Total consumption of ink on startup：3_[Y], [PRINT]S_1252635155, M_94523693, L_2491377016, [FLASH]S_0, M_0, L_107017600
Total consumption of ink on startup：8_[W], [PRINT]S_16542616557, M_15530439, L_5732191, [FLASH]S_0, M_0, L_214028800
Total consumption of ink on startup：9_[V], [PRINT]S_397627, M_285888, L_2907056, [FLASH]S_0, M_0, L_107020800
Total consumption of ink on startup：10_[V1], [PRINT]S_372919, M_292454, L_2865702, [FLASH]S_0, M_0, L_107020800
墨点大小,SMB:3.500000-6.000000-8.000000
data[type=2,serial=007D503240501609202508042010390014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042011100015] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042012110016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042013120017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042014130018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042015140019] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042016150020] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042017160021] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000002, len=392] via MB FAILED, 剩余:3
push data[type=2, serial=MBCP00000003, len=1113] via MB FAILED, 剩余:2
data[type=2, serial=007D503240501609202508042010390014] 重入待发送队列
push data[type=2, serial=MBCP00000004, len=1113] via MB FAILED, 剩余:2
data[type=2, serial=007D503240501609202508042010390014] 重入待发送队列
iot_status:0
push data[type=2, serial=MBCP00000005, len=1113] via MB FAILED, 剩余:2
data[type=2, serial=007D503240501609202508042010390014] 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_556395221, M_984240278, L_980896287, [FLASH]S_0, M_0, L_111883200
Total consumption of ink on startup：1_[C], [PRINT]S_1988019248, M_892470789, L_386076027, [FLASH]S_0, M_0, L_111883200
Total consumption of ink on startup：2_[M], [PRINT]S_1047852143, M_751964316, L_1611781995, [FLASH]S_0, M_0, L_111883200
Total consumption of ink on startup：3_[Y], [PRINT]S_1252635155, M_94523693, L_2491377016, [FLASH]S_0, M_0, L_111883200
Total consumption of ink on startup：8_[W], [PRINT]S_16542616557, M_15530439, L_5732191, [FLASH]S_0, M_0, L_223763200
Total consumption of ink on startup：9_[V], [PRINT]S_397627, M_285888, L_2907056, [FLASH]S_0, M_0, L_111884800
Total consumption of ink on startup：10_[V1], [PRINT]S_372919, M_292454, L_2865702, [FLASH]S_0, M_0, L_111884800
HTTP丢包率：1/1
data[type=512,serial=007D503240501609202508042018170022] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_556425429, M_984263974, L_981138522, [FLASH]S_0, M_0, L_111883200
Total consumption of ink on startup：1_[C], [PRINT]S_1988048608, M_892494709, L_386313555, [FLASH]S_0, M_0, L_111883200
Total consumption of ink on startup：2_[M], [PRINT]S_1047881759, M_751987980, L_1612019523, [FLASH]S_0, M_0, L_111883200
Total consumption of ink on startup：3_[Y], [PRINT]S_1252664195, M_94547933, L_2491614544, [FLASH]S_0, M_0, L_111883200
Total consumption of ink on startup：8_[W], [PRINT]S_16542675077, M_15578791, L_6209661, [FLASH]S_0, M_0, L_223763200
Total consumption of ink on startup：9_[V], [PRINT]S_427239, M_309712, L_3149332, [FLASH]S_0, M_0, L_111884800
Total consumption of ink on startup：10_[V1], [PRINT]S_402211, M_316598, L_3104311, [FLASH]S_0, M_0, L_111884800
墨点大小,SMB:3.500000-6.000000-8.000000
data[type=2,serial=007D503240501609202508042018250023] 入待发送队列
iot_status:0
push data[type=2, serial=MBCP00000006, len=1113] via MB SUCCESSED, 剩余:4
iot_status:3
iot_status:3
iot_status:3
wait data[type=2, serial=007D503240501609202508042018250023] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=007D503240501609202508042019100024] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042019180025] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042020190026] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042021200027] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042022210028] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042023220029] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042024230030] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042025240031] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042026250032] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042027260033] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042028270034] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042029280035] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=007D503240501609202508042058470036] 入待发送队列
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
