云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507040829580000] 入待发送队列
data[type=256,serial=006EA1B2C3D4E5202507040829580001] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_1720, M_1720, L_1720
Total consumption of ink on startup：1_[C], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_1720, M_1720, L_1720
Total consumption of ink on startup：2_[M], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_1720, M_1720, L_1720
Total consumption of ink on startup：3_[Y], [PRINT]S_4800, M_4800, L_4800, [FLASH]S_1720, M_1720, L_1720
Total consumption of ink on startup：4_[W], [PRINT]S_19200, M_19200, L_19200, [FLASH]S_6880, M_6880, L_6880
iot_ccid:CCID-123, imei:IMEI-123
push data[type=256, serial=MBCP00000001, len=468] via MB SUCCESSED, 剩余:1
data[type=128,serial=006EA1B2C3D4E5202507040829580002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507040829580001,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507040829580002,提交成功(0)
push data[type=512, serial=MBCP00000003, len=386] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507040829580000,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507040830590003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507040830590003,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202507040832000004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507040832000004,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041717520000] 入待发送队列
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041718530001] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041719540002] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041720550003] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041721560004] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500101202507041722370005] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041722570006] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041723580007] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041724590008] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041726000009] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041727010010] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500101202507041727440011] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041728020012] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041729030013] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041730040014] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041731050015] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041732060016] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041733070017] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041734080018] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041735090019] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041736100020] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041737110021] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041738120022] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041739130023] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041740140024] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041741150025] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041742160026] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041743170027] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041744180028] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041745190029] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041746200030] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041747210031] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041748220032] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041749230033] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041750240034] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041751250035] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041752260036] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041753270037] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041754280038] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041755290039] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041756300040] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041757310041] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041758320042] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041759330043] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041800340044] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041801350045] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041802360046] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:9.997227-9.997227-19.994453
data[type=1,serial=00F4503250500101202507041803090048] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
墨点大小,SMB:9.997227-9.997227-19.994453
data[type=2,serial=00F4503250500101202507041803260049] 入待发送队列
data[type=4,serial=00F4503250500101202507041803260050] 入待发送队列
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041803370051] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041804380052] 入待发送队列
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041826180053] 入待发送队列
data[type=4,serial=00F4503250500101202507041826180054] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041827190055] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
墨点大小,SMB:9.997227-9.997227-19.994453
data[type=2,serial=00F4503250500101202507041827410056] 入待发送队列
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041828200057] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041829210058] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041830220059] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500101202507041831180060] 入待发送队列
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041831230061] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041832240062] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041833250063] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041834260064] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041849040000] 入待发送队列
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041850050001] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041851060002] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041852070003] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041853080004] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500101202507041853490005] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041854090006] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041855100007] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041856110008] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041857120009] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:9.997227-9.997227-19.994453
data[type=2,serial=00F4503250500101202507041857290010] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041858130011] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041859140012] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041900150013] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041901160014] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041902170015] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041904190017] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:9.997227-9.997227-19.994453
data[type=2,serial=00F4503250500101202507041905080018] 入待发送队列
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041905200019] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041906210020] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041907220021] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041908230022] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041909240023] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041910250024] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041911260025] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500101202507041912270026] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
