云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：4_[Lc], [PRINT]S_0, M_0, L_0, [FLASH]S_80, M_80, L_80
Total consumption of ink on startup：5_[Lm], [PRINT]S_0, M_0, L_0, [FLASH]S_80, M_80, L_80
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202506180901030000] 入待发送队列
data[type=256,serial=006EA1B2C3D4E5202506180901030001] 入待发送队列
push data[type=256, serial=MBCP00000001, len=468] via MB SUCCESSED, 剩余:1
iot_ccid:CCID-123, imei:IMEI-123
data[type=128,serial=006EA1B2C3D4E5202506180901030002] 入待发送队列
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180901030001,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180901030002,提交成功(0)
push data[type=512, serial=MBCP00000003, len=386] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180901030000,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202506180902040003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180902040003,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202506180903050004] 入待发送队列
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180903050004,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202506180904060005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180904060005,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202506180905070006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180905070006,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/7
data[type=512,serial=006EA1B2C3D4E5202506180906080007] 入待发送队列
push data[type=512, serial=MBCP00000008, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180906080007,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
data[type=4,serial=006EA1B2C3D4E5202506180907000008] 入待发送队列
push data[type=4, serial=MBCP00000009, len=418] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
运行状态数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180907000008,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/9
data[type=512,serial=006EA1B2C3D4E5202506180907090009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180907090009,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/10
data[type=512,serial=006EA1B2C3D4E5202506180908100010] 入待发送队列
push data[type=512, serial=MBCP00000011, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180908100010,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202506180908350000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_4200, M_4200, L_4200, [FLASH]S_1340, M_1340, L_1340
Total consumption of ink on startup：1_[C], [PRINT]S_800, M_800, L_800, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：2_[M], [PRINT]S_800, M_800, L_800, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：3_[Y], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_560, M_560, L_560
Total consumption of ink on startup：4_[Lc], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_640, M_640, L_640
Total consumption of ink on startup：5_[Lm], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_640, M_640, L_640
Total consumption of ink on startup：0_[K], [PRINT]S_6300, M_6300, L_6300, [FLASH]S_1340, M_1340, L_1340
Total consumption of ink on startup：1_[C], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：2_[M], [PRINT]S_1200, M_1200, L_1200, [FLASH]S_320, M_320, L_320
Total consumption of ink on startup：3_[Y], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_560, M_560, L_560
Total consumption of ink on startup：4_[Lc], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_640, M_640, L_640
Total consumption of ink on startup：5_[Lm], [PRINT]S_2400, M_2400, L_2400, [FLASH]S_640, M_640, L_640
iot_status:0
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180908350000,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_ccid:CCID-123, imei:IMEI-123
data[type=256,serial=006EA1B2C3D4E5202506180909350001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202506180909350002] 入待发送队列
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180909350002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
HTTP丢包率：1/3
data[type=512,serial=006EA1B2C3D4E5202506180909360003] 入待发送队列
iot_status:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180909350001,提交成功(0)
push data[type=512, serial=MBCP00000004, len=414] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180909360003,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202506180910370004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180910370004,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202506180911380005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180911380005,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202506180912390006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180912390006,提交成功(0)
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_8400, M_8400, L_8400, [FLASH]S_2600, M_2600, L_2600
Total consumption of ink on startup：1_[C], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_560, M_560, L_560
Total consumption of ink on startup：2_[M], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_560, M_560, L_560
Total consumption of ink on startup：3_[Y], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1040, M_1040, L_1040
Total consumption of ink on startup：4_[Lc], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1120, M_1120, L_1120
Total consumption of ink on startup：5_[Lm], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1120, M_1120, L_1120
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202506180913000000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_10500, M_10500, L_10500, [FLASH]S_2600, M_2600, L_2600
Total consumption of ink on startup：1_[C], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_560, M_560, L_560
Total consumption of ink on startup：2_[M], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_560, M_560, L_560
Total consumption of ink on startup：3_[Y], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_1040, M_1040, L_1040
Total consumption of ink on startup：4_[Lc], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_1120, M_1120, L_1120
Total consumption of ink on startup：5_[Lm], [PRINT]S_4000, M_4000, L_4000, [FLASH]S_1120, M_1120, L_1120
iot_status:0
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506180913000000,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181128310000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_1954, M_2180, L_2191, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：1_[C], [PRINT]S_1943, M_2213, L_2281, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：2_[M], [PRINT]S_1937, M_2120, L_2327, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：3_[Y], [PRINT]S_1467, M_1829, L_1768, [FLASH]S_0, M_0, L_51232000
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181129320001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_1954, M_2180, L_2191, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：1_[C], [PRINT]S_1943, M_2213, L_2281, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：2_[M], [PRINT]S_1937, M_2120, L_2327, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：3_[Y], [PRINT]S_1467, M_1829, L_1768, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：0_[K], [PRINT]S_3022, M_3276, L_355959, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：1_[C], [PRINT]S_3007, M_3453, L_348457, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：2_[M], [PRINT]S_3001, M_3376, L_348487, [FLASH]S_0, M_0, L_51232000
Total consumption of ink on startup：3_[Y], [PRINT]S_2577, M_2964, L_348191, [FLASH]S_0, M_0, L_51232000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181130260002] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181130330003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=391] via MB SUCCESSED, 剩余:1
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181130330003] 响应超时(20), 丢弃
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181131340004] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000002, len=391] via MB SUCCESSED, 剩余:1
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181131340004] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181132350005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250104890202506181133220006] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181133360007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181134370008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181135380009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181136390010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181137400011] 入待发送队列
iot_status:3
iot_status:3
data[type=4,serial=0014203250104890202506181140450013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181141420014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_3022, M_3276, L_355959, [FLASH]S_0, M_0, L_64057600
Total consumption of ink on startup：1_[C], [PRINT]S_3007, M_3453, L_348457, [FLASH]S_0, M_0, L_64057600
Total consumption of ink on startup：2_[M], [PRINT]S_3001, M_3376, L_348487, [FLASH]S_0, M_0, L_64057600
Total consumption of ink on startup：3_[Y], [PRINT]S_2577, M_2964, L_348191, [FLASH]S_0, M_0, L_64057600
Total consumption of ink on startup：0_[K], [PRINT]S_4090, M_4372, L_709777, [FLASH]S_0, M_0, L_64057600
Total consumption of ink on startup：1_[C], [PRINT]S_4071, M_4693, L_694633, [FLASH]S_0, M_0, L_64057600
Total consumption of ink on startup：2_[M], [PRINT]S_4065, M_4632, L_694647, [FLASH]S_0, M_0, L_64057600
Total consumption of ink on startup：3_[Y], [PRINT]S_3641, M_4060, L_694511, [FLASH]S_0, M_0, L_64057600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181142320015] 入待发送队列
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000003, len=950] via MB SUCCESSED, 剩余:4
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181142430016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
wait data[type=2, serial=0014203250104890202506181142320015] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_4210, M_4415, L_709777, [FLASH]S_0, M_0, L_76889600
Total consumption of ink on startup：1_[C], [PRINT]S_4071, M_4693, L_694633, [FLASH]S_0, M_0, L_76889600
Total consumption of ink on startup：2_[M], [PRINT]S_4065, M_4632, L_694647, [FLASH]S_0, M_0, L_76889600
Total consumption of ink on startup：3_[Y], [PRINT]S_3641, M_4060, L_694511, [FLASH]S_0, M_0, L_76889600
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181143440017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76661553, M_62948142, L_24709188, [FLASH]S_0, M_0, L_76889600
Total consumption of ink on startup：1_[C], [PRINT]S_89163057, M_64584386, L_19736731, [FLASH]S_0, M_0, L_76889600
Total consumption of ink on startup：2_[M], [PRINT]S_114589558, M_68551487, L_32430192, [FLASH]S_0, M_0, L_76889600
Total consumption of ink on startup：3_[Y], [PRINT]S_81253874, M_81198050, L_50593045, [FLASH]S_0, M_0, L_76889600
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76661553, M_62948142, L_24709188, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：1_[C], [PRINT]S_89163057, M_64584386, L_19736731, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：2_[M], [PRINT]S_114589558, M_68551487, L_32430192, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：3_[Y], [PRINT]S_81253874, M_81198050, L_50593045, [FLASH]S_0, M_0, L_89718400
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181144450020] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_76661553, M_62948446, L_25742484, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：1_[C], [PRINT]S_95921884, M_64586210, L_20768507, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：2_[M], [PRINT]S_163745090, M_96231995, L_34106143, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：3_[Y], [PRINT]S_96871632, M_81198354, L_51626341, [FLASH]S_0, M_0, L_89718400
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181144450021] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181145460022] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181146470023] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181147480024] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181148490025] 入待发送队列
iot_status:3
data[type=4,serial=0014203250104890202506181148580026] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181149500027] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181150510028] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:0
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181200340000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_76661553, M_62948446, L_25742484, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：1_[C], [PRINT]S_95921884, M_64586210, L_20768507, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：2_[M], [PRINT]S_163745090, M_96231995, L_34106143, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：3_[Y], [PRINT]S_96871632, M_81198354, L_51626341, [FLASH]S_0, M_0, L_89718400
push data[type=512, serial=MBCP00000001, len=391] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181200340000] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181201350001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181202360002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181203370003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181204380004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181206020000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_76661553, M_62948446, L_25742484, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：1_[C], [PRINT]S_95921884, M_64586210, L_20768507, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：2_[M], [PRINT]S_163745090, M_96231995, L_34106143, [FLASH]S_0, M_0, L_89718400
Total consumption of ink on startup：3_[Y], [PRINT]S_96871632, M_81198354, L_51626341, [FLASH]S_0, M_0, L_89718400
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181207030001] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000001, len=391] via MB SUCCESSED, 剩余:0
wait data[type=512, serial=0014203250104890202506181207030001] 响应超时(20), 丢弃
iot_status:0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76661553, M_62948446, L_25742484, [FLASH]S_0, M_0, L_102550400
Total consumption of ink on startup：1_[C], [PRINT]S_95921884, M_64586210, L_20768507, [FLASH]S_0, M_0, L_102550400
Total consumption of ink on startup：2_[M], [PRINT]S_163745090, M_96231995, L_34106143, [FLASH]S_0, M_0, L_102550400
Total consumption of ink on startup：3_[Y], [PRINT]S_96871632, M_81198354, L_51626341, [FLASH]S_0, M_0, L_102550400
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181208040002] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_76662621, M_62949542, L_26096324, [FLASH]S_0, M_0, L_102550400
Total consumption of ink on startup：1_[C], [PRINT]S_95922948, M_64587450, L_21114683, [FLASH]S_0, M_0, L_102550400
Total consumption of ink on startup：2_[M], [PRINT]S_163746154, M_96233251, L_34452303, [FLASH]S_0, M_0, L_102550400
Total consumption of ink on startup：3_[Y], [PRINT]S_96872696, M_81199450, L_51972661, [FLASH]S_0, M_0, L_102550400
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181208110003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000002, len=950] via MB SUCCESSED, 剩余:1
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76662621, M_62949542, L_26096324, [FLASH]S_0, M_0, L_115459200
Total consumption of ink on startup：1_[C], [PRINT]S_95922948, M_64587450, L_21114683, [FLASH]S_0, M_0, L_115459200
Total consumption of ink on startup：2_[M], [PRINT]S_163746154, M_96233251, L_34452303, [FLASH]S_0, M_0, L_115459200
Total consumption of ink on startup：3_[Y], [PRINT]S_96872696, M_81199450, L_51972661, [FLASH]S_0, M_0, L_115459200
iot_status:3
wait data[type=2, serial=0014203250104890202506181208110003] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181209050004] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_76662621, M_62949846, L_27129620, [FLASH]S_0, M_0, L_115459200
Total consumption of ink on startup：1_[C], [PRINT]S_102681775, M_64589274, L_22146459, [FLASH]S_0, M_0, L_115459200
Total consumption of ink on startup：2_[M], [PRINT]S_212901686, M_123913759, L_36128254, [FLASH]S_0, M_0, L_115459200
Total consumption of ink on startup：3_[Y], [PRINT]S_112490454, M_81199754, L_53005957, [FLASH]S_0, M_0, L_115459200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181209130006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76662621, M_62949846, L_27129689, [FLASH]S_0, M_0, L_128297600
Total consumption of ink on startup：1_[C], [PRINT]S_102681775, M_64589274, L_22146459, [FLASH]S_0, M_0, L_128297600
Total consumption of ink on startup：2_[M], [PRINT]S_212901686, M_123913759, L_36128254, [FLASH]S_0, M_0, L_128297600
Total consumption of ink on startup：3_[Y], [PRINT]S_112490454, M_81199754, L_53005957, [FLASH]S_0, M_0, L_128297600
Total consumption of ink on startup：0_[K], [PRINT]S_76663614, M_62950553, L_27321655, [FLASH]S_0, M_0, L_128297600
Total consumption of ink on startup：1_[C], [PRINT]S_102681775, M_64589538, L_22309395, [FLASH]S_0, M_0, L_128297600
Total consumption of ink on startup：2_[M], [PRINT]S_212901686, M_123914047, L_36291166, [FLASH]S_0, M_0, L_128297600
Total consumption of ink on startup：3_[Y], [PRINT]S_112490454, M_81199802, L_53169109, [FLASH]S_0, M_0, L_128297600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181209410008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181210060009] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_76663614, M_62950553, L_27321655, [FLASH]S_0, M_0, L_141136000
Total consumption of ink on startup：1_[C], [PRINT]S_102681775, M_64589538, L_22309395, [FLASH]S_0, M_0, L_141136000
Total consumption of ink on startup：2_[M], [PRINT]S_212901686, M_123914047, L_36291166, [FLASH]S_0, M_0, L_141136000
Total consumption of ink on startup：3_[Y], [PRINT]S_112490454, M_81199802, L_53169109, [FLASH]S_0, M_0, L_141136000
Total consumption of ink on startup：0_[K], [PRINT]S_76699614, M_63285682, L_27524379, [FLASH]S_0, M_0, L_141136000
Total consumption of ink on startup：1_[C], [PRINT]S_102681775, M_64589802, L_22472331, [FLASH]S_0, M_0, L_141136000
Total consumption of ink on startup：2_[M], [PRINT]S_212901686, M_123914335, L_36454078, [FLASH]S_0, M_0, L_141136000
Total consumption of ink on startup：3_[Y], [PRINT]S_112490454, M_81199850, L_53332261, [FLASH]S_0, M_0, L_141136000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181210180010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76699614, M_63285682, L_27524379, [FLASH]S_0, M_0, L_153958400
Total consumption of ink on startup：1_[C], [PRINT]S_102681775, M_64589802, L_22472331, [FLASH]S_0, M_0, L_153958400
Total consumption of ink on startup：2_[M], [PRINT]S_212901686, M_123914335, L_36454078, [FLASH]S_0, M_0, L_153958400
Total consumption of ink on startup：3_[Y], [PRINT]S_112490454, M_81199850, L_53332261, [FLASH]S_0, M_0, L_153958400
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76699614, M_63300049, L_28274070, [FLASH]S_0, M_0, L_153958400
Total consumption of ink on startup：1_[C], [PRINT]S_102681775, M_64590594, L_22961139, [FLASH]S_0, M_0, L_153958400
Total consumption of ink on startup：2_[M], [PRINT]S_212901686, M_123915199, L_36942814, [FLASH]S_0, M_0, L_153958400
Total consumption of ink on startup：3_[Y], [PRINT]S_112490454, M_81199994, L_53821717, [FLASH]S_0, M_0, L_153958400
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181210580011] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181211070012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76699614, M_63300049, L_28274070, [FLASH]S_0, M_0, L_166790400
Total consumption of ink on startup：1_[C], [PRINT]S_102681775, M_64590594, L_22961139, [FLASH]S_0, M_0, L_166790400
Total consumption of ink on startup：2_[M], [PRINT]S_212901686, M_123915199, L_36942814, [FLASH]S_0, M_0, L_166790400
Total consumption of ink on startup：3_[Y], [PRINT]S_112490454, M_81199994, L_53821717, [FLASH]S_0, M_0, L_166790400
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181212080013] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_76699614, M_63300353, L_29307366, [FLASH]S_0, M_0, L_166790400
Total consumption of ink on startup：1_[C], [PRINT]S_109440602, M_64592418, L_23992915, [FLASH]S_0, M_0, L_166790400
Total consumption of ink on startup：2_[M], [PRINT]S_262057218, M_151595707, L_38618765, [FLASH]S_0, M_0, L_166790400
Total consumption of ink on startup：3_[Y], [PRINT]S_128108212, M_81200298, L_54855013, [FLASH]S_0, M_0, L_166790400
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181212110014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181300380015] 入待发送队列
iot_status:3
data[type=4,serial=0014203250104890202506181300410016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76699614, M_63300353, L_29307366, [FLASH]S_0, M_0, L_179619200
Total consumption of ink on startup：1_[C], [PRINT]S_109440602, M_64592418, L_23992915, [FLASH]S_0, M_0, L_179619200
Total consumption of ink on startup：2_[M], [PRINT]S_262057218, M_151595707, L_38618765, [FLASH]S_0, M_0, L_179619200
Total consumption of ink on startup：3_[Y], [PRINT]S_128108212, M_81200298, L_54855013, [FLASH]S_0, M_0, L_179619200
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63657394, L_30153777, [FLASH]S_0, M_0, L_179619200
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64898694, L_24533243, [FLASH]S_0, M_0, L_179619200
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151901207, L_39159053, [FLASH]S_0, M_0, L_179619200
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506214, L_55395701, [FLASH]S_0, M_0, L_179619200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181301270017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181301390018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000003, len=391] via MB SUCCESSED, 剩余:10
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181301390018] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181302400019] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181323190000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63657394, L_30153777, [FLASH]S_0, M_0, L_179619200
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64898694, L_24533243, [FLASH]S_0, M_0, L_179619200
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151901207, L_39159053, [FLASH]S_0, M_0, L_179619200
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506214, L_55395701, [FLASH]S_0, M_0, L_179619200
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181324200001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63657394, L_30153777, [FLASH]S_0, M_0, L_192441600
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64898694, L_24533243, [FLASH]S_0, M_0, L_192441600
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151901207, L_39159053, [FLASH]S_0, M_0, L_192441600
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506214, L_55395701, [FLASH]S_0, M_0, L_192441600
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63658996, L_31102943, [FLASH]S_0, M_0, L_192441600
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64899310, L_24913427, [FLASH]S_0, M_0, L_192441600
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151901879, L_39539181, [FLASH]S_0, M_0, L_192441600
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506326, L_55776389, [FLASH]S_0, M_0, L_192441600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181325040002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181325210003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63658996, L_31102943, [FLASH]S_0, M_0, L_205267200
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64899310, L_24913427, [FLASH]S_0, M_0, L_205267200
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151901879, L_39539181, [FLASH]S_0, M_0, L_205267200
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506326, L_55776389, [FLASH]S_0, M_0, L_205267200
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63660598, L_32052091, [FLASH]S_0, M_0, L_205267200
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64899926, L_25293611, [FLASH]S_0, M_0, L_205267200
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151902551, L_39919309, [FLASH]S_0, M_0, L_205267200
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506438, L_56157077, [FLASH]S_0, M_0, L_205267200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181326150004] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181326220005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63660598, L_32052091, [FLASH]S_0, M_0, L_218096000
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64899926, L_25293611, [FLASH]S_0, M_0, L_218096000
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151902551, L_39919309, [FLASH]S_0, M_0, L_218096000
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506438, L_56157077, [FLASH]S_0, M_0, L_218096000
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63662555, L_32294594, [FLASH]S_0, M_0, L_218096000
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64900190, L_25456547, [FLASH]S_0, M_0, L_218096000
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151902839, L_40082221, [FLASH]S_0, M_0, L_218096000
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506486, L_56320229, [FLASH]S_0, M_0, L_218096000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181327050006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181327230007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63662555, L_32294594, [FLASH]S_0, M_0, L_230928000
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64900190, L_25456547, [FLASH]S_0, M_0, L_230928000
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151902839, L_40082221, [FLASH]S_0, M_0, L_230928000
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506486, L_56320229, [FLASH]S_0, M_0, L_230928000
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63676922, L_33044258, [FLASH]S_0, M_0, L_230928000
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64900982, L_25945355, [FLASH]S_0, M_0, L_230928000
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151903703, L_40570957, [FLASH]S_0, M_0, L_230928000
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506630, L_56809685, [FLASH]S_0, M_0, L_230928000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181328100008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181328240009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63676922, L_33044258, [FLASH]S_0, M_0, L_243756800
Total consumption of ink on startup：1_[C], [PRINT]S_109441114, M_64900982, L_25945355, [FLASH]S_0, M_0, L_243756800
Total consumption of ink on startup：2_[M], [PRINT]S_262057730, M_151903703, L_40570957, [FLASH]S_0, M_0, L_243756800
Total consumption of ink on startup：3_[Y], [PRINT]S_128108724, M_81506630, L_56809685, [FLASH]S_0, M_0, L_243756800
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63677226, L_34077554, [FLASH]S_0, M_0, L_243756800
Total consumption of ink on startup：1_[C], [PRINT]S_116199941, M_64902806, L_26977131, [FLASH]S_0, M_0, L_243756800
Total consumption of ink on startup：2_[M], [PRINT]S_311213262, M_179584211, L_42246908, [FLASH]S_0, M_0, L_243756800
Total consumption of ink on startup：3_[Y], [PRINT]S_143726482, M_81506934, L_57842981, [FLASH]S_0, M_0, L_243756800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181329090010] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=0014203250104890202506181329090011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181329250012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181330260013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181331270014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181332280015] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63677226, L_34077554, [FLASH]S_0, M_0, L_256588800
Total consumption of ink on startup：1_[C], [PRINT]S_116199941, M_64902806, L_26977131, [FLASH]S_0, M_0, L_256588800
Total consumption of ink on startup：2_[M], [PRINT]S_311213262, M_179584211, L_42246908, [FLASH]S_0, M_0, L_256588800
Total consumption of ink on startup：3_[Y], [PRINT]S_143726482, M_81506934, L_57842981, [FLASH]S_0, M_0, L_256588800
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_76700142, M_63677466, L_34893314, [FLASH]S_0, M_0, L_256588800
Total consumption of ink on startup：1_[C], [PRINT]S_122958768, M_64904246, L_27791691, [FLASH]S_0, M_0, L_256588800
Total consumption of ink on startup：2_[M], [PRINT]S_360541143, M_207264367, L_43705611, [FLASH]S_0, M_0, L_256588800
Total consumption of ink on startup：3_[Y], [PRINT]S_159344240, M_81507174, L_58658741, [FLASH]S_0, M_0, L_256588800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181333000017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000001, len=957] via MB SUCCESSED, 剩余:8
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181333290018] 入待发送队列
iot_status:3
data[type=4,serial=0014203250104890202506181333380019] 入待发送队列
wait data[type=2, serial=0014203250104890202506181333000017] 响应超时(20), 重入待发送队列
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181334300020] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:0
push data[type=512, serial=MBCP00000002, len=391] via MB SUCCESSED, 剩余:9
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181335310021] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181334300020] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181336320022] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181337330023] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181338340024] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181339350025] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_3418, M_4279, L_3325, [FLASH]S_0, M_0, L_12819200
Total consumption of ink on startup：1_[C], [PRINT]S_3435, M_4264, L_3307, [FLASH]S_0, M_0, L_12819200
Total consumption of ink on startup：2_[M], [PRINT]S_3010, M_3707, L_3058, [FLASH]S_0, M_0, L_12819200
Total consumption of ink on startup：3_[Y], [PRINT]S_2971, M_3796, L_2992, [FLASH]S_0, M_0, L_12819200
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_3946, M_361320, L_849743, [FLASH]S_0, M_0, L_12819200
Total consumption of ink on startup：1_[C], [PRINT]S_3947, M_310540, L_543635, [FLASH]S_0, M_0, L_12819200
Total consumption of ink on startup：2_[M], [PRINT]S_3522, M_309207, L_543346, [FLASH]S_0, M_0, L_12819200
Total consumption of ink on startup：3_[Y], [PRINT]S_3483, M_309712, L_543680, [FLASH]S_0, M_0, L_12819200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181340240026] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181340360027] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181341370028] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181342380029] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_3946, M_361320, L_849743, [FLASH]S_0, M_0, L_25644800
Total consumption of ink on startup：1_[C], [PRINT]S_3947, M_310540, L_543635, [FLASH]S_0, M_0, L_25644800
Total consumption of ink on startup：2_[M], [PRINT]S_3522, M_309207, L_543346, [FLASH]S_0, M_0, L_25644800
Total consumption of ink on startup：3_[Y], [PRINT]S_3483, M_309712, L_543680, [FLASH]S_0, M_0, L_25644800
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_4474, M_718361, L_1696205, [FLASH]S_0, M_0, L_25644800
Total consumption of ink on startup：1_[C], [PRINT]S_4459, M_616816, L_1083963, [FLASH]S_0, M_0, L_25644800
Total consumption of ink on startup：2_[M], [PRINT]S_4034, M_614707, L_1083634, [FLASH]S_0, M_0, L_25644800
Total consumption of ink on startup：3_[Y], [PRINT]S_3995, M_615628, L_1084368, [FLASH]S_0, M_0, L_25644800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181343250030] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181343390031] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181344400032] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_4474, M_718361, L_1696205, [FLASH]S_0, M_0, L_38457600
Total consumption of ink on startup：1_[C], [PRINT]S_4459, M_616816, L_1083963, [FLASH]S_0, M_0, L_38457600
Total consumption of ink on startup：2_[M], [PRINT]S_4034, M_614707, L_1083634, [FLASH]S_0, M_0, L_38457600
Total consumption of ink on startup：3_[Y], [PRINT]S_3995, M_615628, L_1084368, [FLASH]S_0, M_0, L_38457600
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181345410033] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5002, M_1075402, L_2542661, [FLASH]S_0, M_0, L_38457600
Total consumption of ink on startup：1_[C], [PRINT]S_4971, M_923092, L_1624291, [FLASH]S_0, M_0, L_38457600
Total consumption of ink on startup：2_[M], [PRINT]S_4546, M_920207, L_1623922, [FLASH]S_0, M_0, L_38457600
Total consumption of ink on startup：3_[Y], [PRINT]S_4507, M_921544, L_1625056, [FLASH]S_0, M_0, L_38457600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181345530034] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181346420035] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181347430036] 入待发送队列
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181351240000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_5002, M_1075402, L_2542661, [FLASH]S_0, M_0, L_38457600
Total consumption of ink on startup：1_[C], [PRINT]S_4971, M_923092, L_1624291, [FLASH]S_0, M_0, L_38457600
Total consumption of ink on startup：2_[M], [PRINT]S_4546, M_920207, L_1623922, [FLASH]S_0, M_0, L_38457600
Total consumption of ink on startup：3_[Y], [PRINT]S_4507, M_921544, L_1625056, [FLASH]S_0, M_0, L_38457600
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5002, M_1075402, L_2542661, [FLASH]S_0, M_0, L_51280000
Total consumption of ink on startup：1_[C], [PRINT]S_4971, M_923092, L_1624291, [FLASH]S_0, M_0, L_51280000
Total consumption of ink on startup：2_[M], [PRINT]S_4546, M_920207, L_1623922, [FLASH]S_0, M_0, L_51280000
Total consumption of ink on startup：3_[Y], [PRINT]S_4507, M_921544, L_1625056, [FLASH]S_0, M_0, L_51280000
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5530, M_1432443, L_3389070, [FLASH]S_0, M_0, L_51280000
Total consumption of ink on startup：1_[C], [PRINT]S_5483, M_1229368, L_2164619, [FLASH]S_0, M_0, L_51280000
Total consumption of ink on startup：2_[M], [PRINT]S_5058, M_1225707, L_2164210, [FLASH]S_0, M_0, L_51280000
Total consumption of ink on startup：3_[Y], [PRINT]S_5019, M_1227460, L_2165744, [FLASH]S_0, M_0, L_51280000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181352060001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181352250002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181353260003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181354270004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5530, M_1432443, L_3389070, [FLASH]S_0, M_0, L_64105600
Total consumption of ink on startup：1_[C], [PRINT]S_5483, M_1229368, L_2164619, [FLASH]S_0, M_0, L_64105600
Total consumption of ink on startup：2_[M], [PRINT]S_5058, M_1225707, L_2164210, [FLASH]S_0, M_0, L_64105600
Total consumption of ink on startup：3_[Y], [PRINT]S_5019, M_1227460, L_2165744, [FLASH]S_0, M_0, L_64105600
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181355280005] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_6058, M_1789484, L_4235526, [FLASH]S_0, M_0, L_64105600
Total consumption of ink on startup：1_[C], [PRINT]S_5995, M_1535644, L_2704947, [FLASH]S_0, M_0, L_64105600
Total consumption of ink on startup：2_[M], [PRINT]S_5570, M_1531207, L_2704498, [FLASH]S_0, M_0, L_64105600
Total consumption of ink on startup：3_[Y], [PRINT]S_5531, M_1533376, L_2706432, [FLASH]S_0, M_0, L_64105600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181355360006] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=0014203250104890202506181355360007] 入待发送队列
iot_status:3
iot_status:3
iot_status:0
push data[type=1, serial=MBCP00000001, len=944] via MB SUCCESSED, 剩余:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=1, serial=0014203250104890202506181355360007] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181356290008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181357300009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181358310010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_6058, M_1789484, L_4235526, [FLASH]S_0, M_0, L_76931200
Total consumption of ink on startup：1_[C], [PRINT]S_5995, M_1535644, L_2704947, [FLASH]S_0, M_0, L_76931200
Total consumption of ink on startup：2_[M], [PRINT]S_5570, M_1531207, L_2704498, [FLASH]S_0, M_0, L_76931200
Total consumption of ink on startup：3_[Y], [PRINT]S_5531, M_1533376, L_2706432, [FLASH]S_0, M_0, L_76931200
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_6586, M_2146525, L_5081967, [FLASH]S_0, M_0, L_76931200
Total consumption of ink on startup：1_[C], [PRINT]S_6507, M_1841920, L_3245275, [FLASH]S_0, M_0, L_76931200
Total consumption of ink on startup：2_[M], [PRINT]S_6082, M_1836707, L_3244786, [FLASH]S_0, M_0, L_76931200
Total consumption of ink on startup：3_[Y], [PRINT]S_6043, M_1839292, L_3247120, [FLASH]S_0, M_0, L_76931200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181359210011] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181359320012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181400330013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_6586, M_2146525, L_5081967, [FLASH]S_0, M_0, L_89756800
Total consumption of ink on startup：1_[C], [PRINT]S_6507, M_1841920, L_3245275, [FLASH]S_0, M_0, L_89756800
Total consumption of ink on startup：2_[M], [PRINT]S_6082, M_1836707, L_3244786, [FLASH]S_0, M_0, L_89756800
Total consumption of ink on startup：3_[Y], [PRINT]S_6043, M_1839292, L_3247120, [FLASH]S_0, M_0, L_89756800
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181401340014] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_7114, M_2503566, L_5928342, [FLASH]S_0, M_0, L_89756800
Total consumption of ink on startup：1_[C], [PRINT]S_7019, M_2148196, L_3785603, [FLASH]S_0, M_0, L_89756800
Total consumption of ink on startup：2_[M], [PRINT]S_6594, M_2142207, L_3785074, [FLASH]S_0, M_0, L_89756800
Total consumption of ink on startup：3_[Y], [PRINT]S_6555, M_2145208, L_3787808, [FLASH]S_0, M_0, L_89756800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181401420015] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181402350016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181403360017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181404370018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181405380019] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181406390020] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_7114, M_2503566, L_5928342, [FLASH]S_0, M_0, L_102582400
Total consumption of ink on startup：1_[C], [PRINT]S_7019, M_2148196, L_3785603, [FLASH]S_0, M_0, L_102582400
Total consumption of ink on startup：2_[M], [PRINT]S_6594, M_2142207, L_3785074, [FLASH]S_0, M_0, L_102582400
Total consumption of ink on startup：3_[Y], [PRINT]S_6555, M_2145208, L_3787808, [FLASH]S_0, M_0, L_102582400
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181407400021] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_7642, M_2860607, L_6774751, [FLASH]S_0, M_0, L_102582400
Total consumption of ink on startup：1_[C], [PRINT]S_7531, M_2454472, L_4325931, [FLASH]S_0, M_0, L_102582400
Total consumption of ink on startup：2_[M], [PRINT]S_7106, M_2447707, L_4325362, [FLASH]S_0, M_0, L_102582400
Total consumption of ink on startup：3_[Y], [PRINT]S_7067, M_2451124, L_4328496, [FLASH]S_0, M_0, L_102582400
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181407510022] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181408410023] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000002, len=391] via MB SUCCESSED, 剩余:5
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181408410023] 响应超时(20), 丢弃
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181409420024] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181410430025] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_7642, M_2860607, L_6774751, [FLASH]S_0, M_0, L_115414400
Total consumption of ink on startup：1_[C], [PRINT]S_7531, M_2454472, L_4325931, [FLASH]S_0, M_0, L_115414400
Total consumption of ink on startup：2_[M], [PRINT]S_7106, M_2447707, L_4325362, [FLASH]S_0, M_0, L_115414400
Total consumption of ink on startup：3_[Y], [PRINT]S_7067, M_2451124, L_4328496, [FLASH]S_0, M_0, L_115414400
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_8170, M_3217648, L_7621159, [FLASH]S_0, M_0, L_115414400
Total consumption of ink on startup：1_[C], [PRINT]S_8043, M_2760748, L_4866259, [FLASH]S_0, M_0, L_115414400
Total consumption of ink on startup：2_[M], [PRINT]S_7618, M_2753207, L_4865650, [FLASH]S_0, M_0, L_115414400
Total consumption of ink on startup：3_[Y], [PRINT]S_7579, M_2757040, L_4869184, [FLASH]S_0, M_0, L_115414400
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181411060026] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181411440027] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181412450028] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_8170, M_3217648, L_7621159, [FLASH]S_0, M_0, L_128236800
Total consumption of ink on startup：1_[C], [PRINT]S_8043, M_2760748, L_4866259, [FLASH]S_0, M_0, L_128236800
Total consumption of ink on startup：2_[M], [PRINT]S_7618, M_2753207, L_4865650, [FLASH]S_0, M_0, L_128236800
Total consumption of ink on startup：3_[Y], [PRINT]S_7579, M_2757040, L_4869184, [FLASH]S_0, M_0, L_128236800
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_8698, M_3574689, L_8467559, [FLASH]S_0, M_0, L_128236800
Total consumption of ink on startup：1_[C], [PRINT]S_8555, M_3067024, L_5406587, [FLASH]S_0, M_0, L_128236800
Total consumption of ink on startup：2_[M], [PRINT]S_8130, M_3058707, L_5405938, [FLASH]S_0, M_0, L_128236800
Total consumption of ink on startup：3_[Y], [PRINT]S_8091, M_3062956, L_5409872, [FLASH]S_0, M_0, L_128236800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181413100029] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181413460030] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181414470031] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_8698, M_3574689, L_8467559, [FLASH]S_0, M_0, L_141097600
Total consumption of ink on startup：1_[C], [PRINT]S_8555, M_3067024, L_5406587, [FLASH]S_0, M_0, L_141097600
Total consumption of ink on startup：2_[M], [PRINT]S_8130, M_3058707, L_5405938, [FLASH]S_0, M_0, L_141097600
Total consumption of ink on startup：3_[Y], [PRINT]S_8091, M_3062956, L_5409872, [FLASH]S_0, M_0, L_141097600
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_9226, M_3931730, L_9313951, [FLASH]S_0, M_0, L_141097600
Total consumption of ink on startup：1_[C], [PRINT]S_9067, M_3373300, L_5946915, [FLASH]S_0, M_0, L_141097600
Total consumption of ink on startup：2_[M], [PRINT]S_8642, M_3364207, L_5946226, [FLASH]S_0, M_0, L_141097600
Total consumption of ink on startup：3_[Y], [PRINT]S_8603, M_3368872, L_5950560, [FLASH]S_0, M_0, L_141097600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181415310032] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181415480033] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_9226, M_3931730, L_9313951, [FLASH]S_0, M_0, L_153926400
Total consumption of ink on startup：1_[C], [PRINT]S_9067, M_3373300, L_5946915, [FLASH]S_0, M_0, L_153926400
Total consumption of ink on startup：2_[M], [PRINT]S_8642, M_3364207, L_5946226, [FLASH]S_0, M_0, L_153926400
Total consumption of ink on startup：3_[Y], [PRINT]S_8603, M_3368872, L_5950560, [FLASH]S_0, M_0, L_153926400
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181416490034] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_9754, M_4288771, L_10160318, [FLASH]S_0, M_0, L_153926400
Total consumption of ink on startup：1_[C], [PRINT]S_9579, M_3679576, L_6487243, [FLASH]S_0, M_0, L_153926400
Total consumption of ink on startup：2_[M], [PRINT]S_9154, M_3669707, L_6486514, [FLASH]S_0, M_0, L_153926400
Total consumption of ink on startup：3_[Y], [PRINT]S_9115, M_3674788, L_6491248, [FLASH]S_0, M_0, L_153926400
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181416580035] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181417500036] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000003, len=391] via MB SUCCESSED, 剩余:9
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181418510037] 入待发送队列
iot_status:3
wait data[type=512, serial=0014203250104890202506181417500036] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_9754, M_4288771, L_10160318, [FLASH]S_0, M_0, L_166752000
Total consumption of ink on startup：1_[C], [PRINT]S_9579, M_3679576, L_6487243, [FLASH]S_0, M_0, L_166752000
Total consumption of ink on startup：2_[M], [PRINT]S_9154, M_3669707, L_6486514, [FLASH]S_0, M_0, L_166752000
Total consumption of ink on startup：3_[Y], [PRINT]S_9115, M_3674788, L_6491248, [FLASH]S_0, M_0, L_166752000
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_10282, M_4645812, L_11006725, [FLASH]S_0, M_0, L_166752000
Total consumption of ink on startup：1_[C], [PRINT]S_10091, M_3985852, L_7027571, [FLASH]S_0, M_0, L_166752000
Total consumption of ink on startup：2_[M], [PRINT]S_9666, M_3975207, L_7026802, [FLASH]S_0, M_0, L_166752000
Total consumption of ink on startup：3_[Y], [PRINT]S_9627, M_3980704, L_7031936, [FLASH]S_0, M_0, L_166752000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181419220038] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181419520039] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181420530040] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_10282, M_4645812, L_11006725, [FLASH]S_0, M_0, L_179577600
Total consumption of ink on startup：1_[C], [PRINT]S_10091, M_3985852, L_7027571, [FLASH]S_0, M_0, L_179577600
Total consumption of ink on startup：2_[M], [PRINT]S_9666, M_3975207, L_7026802, [FLASH]S_0, M_0, L_179577600
Total consumption of ink on startup：3_[Y], [PRINT]S_9627, M_3980704, L_7031936, [FLASH]S_0, M_0, L_179577600
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181421540041] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_10810, M_5002853, L_11853114, [FLASH]S_0, M_0, L_179577600
Total consumption of ink on startup：1_[C], [PRINT]S_10603, M_4292128, L_7567899, [FLASH]S_0, M_0, L_179577600
Total consumption of ink on startup：2_[M], [PRINT]S_10178, M_4280707, L_7567090, [FLASH]S_0, M_0, L_179577600
Total consumption of ink on startup：3_[Y], [PRINT]S_10139, M_4286620, L_7572624, [FLASH]S_0, M_0, L_179577600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181422030042] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181422550043] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181423560044] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_10810, M_5002853, L_11853114, [FLASH]S_0, M_0, L_192403200
Total consumption of ink on startup：1_[C], [PRINT]S_10603, M_4292128, L_7567899, [FLASH]S_0, M_0, L_192403200
Total consumption of ink on startup：2_[M], [PRINT]S_10178, M_4280707, L_7567090, [FLASH]S_0, M_0, L_192403200
Total consumption of ink on startup：3_[Y], [PRINT]S_10139, M_4286620, L_7572624, [FLASH]S_0, M_0, L_192403200
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_11338, M_5359894, L_12699564, [FLASH]S_0, M_0, L_192403200
Total consumption of ink on startup：1_[C], [PRINT]S_11115, M_4598404, L_8108227, [FLASH]S_0, M_0, L_192403200
Total consumption of ink on startup：2_[M], [PRINT]S_10690, M_4586207, L_8107378, [FLASH]S_0, M_0, L_192403200
Total consumption of ink on startup：3_[Y], [PRINT]S_10651, M_4592536, L_8113312, [FLASH]S_0, M_0, L_192403200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181424130045] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_11338, M_5359894, L_12699564, [FLASH]S_0, M_0, L_205216000
Total consumption of ink on startup：1_[C], [PRINT]S_11115, M_4598404, L_8108227, [FLASH]S_0, M_0, L_205216000
Total consumption of ink on startup：2_[M], [PRINT]S_10690, M_4586207, L_8107378, [FLASH]S_0, M_0, L_205216000
Total consumption of ink on startup：3_[Y], [PRINT]S_10651, M_4592536, L_8113312, [FLASH]S_0, M_0, L_205216000
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_11866, M_5716935, L_13545983, [FLASH]S_0, M_0, L_205216000
Total consumption of ink on startup：1_[C], [PRINT]S_11627, M_4904680, L_8648555, [FLASH]S_0, M_0, L_205216000
Total consumption of ink on startup：2_[M], [PRINT]S_11202, M_4891707, L_8647666, [FLASH]S_0, M_0, L_205216000
Total consumption of ink on startup：3_[Y], [PRINT]S_11163, M_4898452, L_8654000, [FLASH]S_0, M_0, L_205216000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181424430046] 入待发送队列
iot_status:0
push data[type=2, serial=MBCP00000004, len=944] via MB SUCCESSED, 剩余:13
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181424570047] 入待发送队列
iot_status:3
iot_status:3
wait data[type=2, serial=0014203250104890202506181424430046] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181425580048] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181426590049] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181428000050] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_11866, M_5716935, L_13545983, [FLASH]S_0, M_0, L_218048000
Total consumption of ink on startup：1_[C], [PRINT]S_11627, M_4904680, L_8648555, [FLASH]S_0, M_0, L_218048000
Total consumption of ink on startup：2_[M], [PRINT]S_11202, M_4891707, L_8647666, [FLASH]S_0, M_0, L_218048000
Total consumption of ink on startup：3_[Y], [PRINT]S_11163, M_4898452, L_8654000, [FLASH]S_0, M_0, L_218048000
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_12394, M_6073976, L_14392387, [FLASH]S_0, M_0, L_218048000
Total consumption of ink on startup：1_[C], [PRINT]S_12139, M_5210956, L_9188883, [FLASH]S_0, M_0, L_218048000
Total consumption of ink on startup：2_[M], [PRINT]S_11714, M_5197207, L_9187954, [FLASH]S_0, M_0, L_218048000
Total consumption of ink on startup：3_[Y], [PRINT]S_11675, M_5204368, L_9194688, [FLASH]S_0, M_0, L_218048000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181428380051] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181429010052] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181430020053] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181431030054] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_12394, M_6073976, L_14392387, [FLASH]S_0, M_0, L_230873600
Total consumption of ink on startup：1_[C], [PRINT]S_12139, M_5210956, L_9188883, [FLASH]S_0, M_0, L_230873600
Total consumption of ink on startup：2_[M], [PRINT]S_11714, M_5197207, L_9187954, [FLASH]S_0, M_0, L_230873600
Total consumption of ink on startup：3_[Y], [PRINT]S_11675, M_5204368, L_9194688, [FLASH]S_0, M_0, L_230873600
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_12922, M_6431017, L_15238777, [FLASH]S_0, M_0, L_230873600
Total consumption of ink on startup：1_[C], [PRINT]S_12651, M_5517232, L_9729211, [FLASH]S_0, M_0, L_230873600
Total consumption of ink on startup：2_[M], [PRINT]S_12226, M_5502707, L_9728242, [FLASH]S_0, M_0, L_230873600
Total consumption of ink on startup：3_[Y], [PRINT]S_12187, M_5510284, L_9735376, [FLASH]S_0, M_0, L_230873600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181431520055] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181432040056] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181433050057] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_12922, M_6431017, L_15238777, [FLASH]S_0, M_0, L_243692800
Total consumption of ink on startup：1_[C], [PRINT]S_12651, M_5517232, L_9729211, [FLASH]S_0, M_0, L_243692800
Total consumption of ink on startup：2_[M], [PRINT]S_12226, M_5502707, L_9728242, [FLASH]S_0, M_0, L_243692800
Total consumption of ink on startup：3_[Y], [PRINT]S_12187, M_5510284, L_9735376, [FLASH]S_0, M_0, L_243692800
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181434060058] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_13450, M_6788058, L_16085196, [FLASH]S_0, M_0, L_243692800
Total consumption of ink on startup：1_[C], [PRINT]S_13163, M_5823508, L_10269539, [FLASH]S_0, M_0, L_243692800
Total consumption of ink on startup：2_[M], [PRINT]S_12738, M_5808207, L_10268530, [FLASH]S_0, M_0, L_243692800
Total consumption of ink on startup：3_[Y], [PRINT]S_12699, M_5816200, L_10276064, [FLASH]S_0, M_0, L_243692800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181434200059] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181435070060] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181436080061] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_13450, M_6788058, L_16085196, [FLASH]S_0, M_0, L_256521600
Total consumption of ink on startup：1_[C], [PRINT]S_13163, M_5823508, L_10269539, [FLASH]S_0, M_0, L_256521600
Total consumption of ink on startup：2_[M], [PRINT]S_12738, M_5808207, L_10268530, [FLASH]S_0, M_0, L_256521600
Total consumption of ink on startup：3_[Y], [PRINT]S_12699, M_5816200, L_10276064, [FLASH]S_0, M_0, L_256521600
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_13978, M_7145099, L_16931597, [FLASH]S_0, M_0, L_256521600
Total consumption of ink on startup：1_[C], [PRINT]S_13675, M_6129784, L_10809867, [FLASH]S_0, M_0, L_256521600
Total consumption of ink on startup：2_[M], [PRINT]S_13250, M_6113707, L_10808818, [FLASH]S_0, M_0, L_256521600
Total consumption of ink on startup：3_[Y], [PRINT]S_13211, M_6122116, L_10816752, [FLASH]S_0, M_0, L_256521600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181436440062] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181437090063] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_13978, M_7145099, L_16931597, [FLASH]S_0, M_0, L_269347200
Total consumption of ink on startup：1_[C], [PRINT]S_13675, M_6129784, L_10809867, [FLASH]S_0, M_0, L_269347200
Total consumption of ink on startup：2_[M], [PRINT]S_13250, M_6113707, L_10808818, [FLASH]S_0, M_0, L_269347200
Total consumption of ink on startup：3_[Y], [PRINT]S_13211, M_6122116, L_10816752, [FLASH]S_0, M_0, L_269347200
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_14506, M_7502140, L_17778018, [FLASH]S_0, M_0, L_269347200
Total consumption of ink on startup：1_[C], [PRINT]S_14187, M_6436060, L_11350195, [FLASH]S_0, M_0, L_269347200
Total consumption of ink on startup：2_[M], [PRINT]S_13762, M_6419207, L_11349106, [FLASH]S_0, M_0, L_269347200
Total consumption of ink on startup：3_[Y], [PRINT]S_13723, M_6428032, L_11357440, [FLASH]S_0, M_0, L_269347200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181438090064] 入待发送队列
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181438100065] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000005, len=391] via MB SUCCESSED, 剩余:18
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181438100065] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=0014203250104890202506181439110066] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_14506, M_7502140, L_17778018, [FLASH]S_0, M_0, L_282169600
Total consumption of ink on startup：1_[C], [PRINT]S_14187, M_6436060, L_11350195, [FLASH]S_0, M_0, L_282169600
Total consumption of ink on startup：2_[M], [PRINT]S_13762, M_6419207, L_11349106, [FLASH]S_0, M_0, L_282169600
Total consumption of ink on startup：3_[Y], [PRINT]S_13723, M_6428032, L_11357440, [FLASH]S_0, M_0, L_282169600
iot_status:0
push data[type=512, serial=MBCP00000006, len=391] via MB SUCCESSED, 剩余:18
HTTP丢包率：6/6
data[type=512,serial=0014203250104890202506181440120067] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7859181, L_18624452, [FLASH]S_0, M_0, L_282169600
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6742336, L_11890523, [FLASH]S_0, M_0, L_282169600
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6724707, L_11889394, [FLASH]S_0, M_0, L_282169600
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6733948, L_11898128, [FLASH]S_0, M_0, L_282169600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181440200068] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181439110066] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=0014203250104890202506181441130069] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7859181, L_18624452, [FLASH]S_0, M_0, L_294976000
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6742336, L_11890523, [FLASH]S_0, M_0, L_294976000
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6724707, L_11889394, [FLASH]S_0, M_0, L_294976000
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6733948, L_11898128, [FLASH]S_0, M_0, L_294976000
iot_status:3
iot_status:3
data[type=4,serial=0014203250104890202506181441530070] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=0014203250104890202506181442140071] 入待发送队列
data[type=2,serial=0014203250104890202506181442390072] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=0014203250104890202506181443150074] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000007, len=391] via MB SUCCESSED, 剩余:22
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181443150074] 响应超时(20), 丢弃
HTTP丢包率：7/7
data[type=512,serial=0014203250104890202506181444160075] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7860783, L_19573571, [FLASH]S_0, M_0, L_307801600
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6742952, L_12270707, [FLASH]S_0, M_0, L_307801600
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6725379, L_12269522, [FLASH]S_0, M_0, L_307801600
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734060, L_12278816, [FLASH]S_0, M_0, L_307801600
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7862385, L_20522683, [FLASH]S_0, M_0, L_307801600
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6743568, L_12650891, [FLASH]S_0, M_0, L_307801600
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6726051, L_12649650, [FLASH]S_0, M_0, L_307801600
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734172, L_12659504, [FLASH]S_0, M_0, L_307801600
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000008, len=919] via MB SUCCESSED, 剩余:23
HTTP丢包率：8/8
data[type=512,serial=0014203250104890202506181445170077] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7862385, L_20522683, [FLASH]S_0, M_0, L_320627200
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6743568, L_12650891, [FLASH]S_0, M_0, L_320627200
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6726051, L_12649650, [FLASH]S_0, M_0, L_320627200
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734172, L_12659504, [FLASH]S_0, M_0, L_320627200
wait data[type=2, serial=0014203250104890202506181444450076] 响应超时(20), 重入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7864342, L_20765209, [FLASH]S_0, M_0, L_320627200
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6743832, L_12813827, [FLASH]S_0, M_0, L_320627200
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6726339, L_12812562, [FLASH]S_0, M_0, L_320627200
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734220, L_12822656, [FLASH]S_0, M_0, L_320627200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181445420078] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=0014203250104890202506181445420079] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=0014203250104890202506181446180080] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7864342, L_20765209, [FLASH]S_0, M_0, L_333452800
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6743832, L_12813827, [FLASH]S_0, M_0, L_333452800
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6726339, L_12812562, [FLASH]S_0, M_0, L_333452800
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734220, L_12822656, [FLASH]S_0, M_0, L_333452800
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7866299, L_21007709, [FLASH]S_0, M_0, L_333452800
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6744096, L_12976763, [FLASH]S_0, M_0, L_333452800
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6726627, L_12975474, [FLASH]S_0, M_0, L_333452800
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734268, L_12985808, [FLASH]S_0, M_0, L_333452800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181446410081] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250104890202506181446530082] 入待发送队列
iot_status:0
push data[type=4, serial=MBCP00000009, len=500] via MB SUCCESSED, 剩余:27
iot_status:3
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181447070083] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7866299, L_21007709, [FLASH]S_0, M_0, L_346275200
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6744096, L_12976763, [FLASH]S_0, M_0, L_346275200
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6726627, L_12975474, [FLASH]S_0, M_0, L_346275200
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734268, L_12985808, [FLASH]S_0, M_0, L_346275200
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7866299, L_21007709, [FLASH]S_0, M_0, L_346275200
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6744096, L_12976763, [FLASH]S_0, M_0, L_346275200
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6726627, L_12975474, [FLASH]S_0, M_0, L_346275200
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734268, L_12985808, [FLASH]S_0, M_0, L_346275200
iot_status:3
wait data[type=4, serial=0014203250104890202506181446530082] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7866299, L_21007709, [FLASH]S_0, M_0, L_359075200
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6744096, L_12976763, [FLASH]S_0, M_0, L_359075200
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6726627, L_12975474, [FLASH]S_0, M_0, L_359075200
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734268, L_12985808, [FLASH]S_0, M_0, L_359075200
iot_status:0
push data[type=4, serial=MBCP00000010, len=500] via MB SUCCESSED, 剩余:29
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7880666, L_21757414, [FLASH]S_0, M_0, L_359075200
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6744888, L_13465571, [FLASH]S_0, M_0, L_359075200
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6727491, L_13464210, [FLASH]S_0, M_0, L_359075200
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734412, L_13475264, [FLASH]S_0, M_0, L_359075200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181447470087] 入待发送队列
iot_status:3
iot_status:3
wait data[type=4, serial=0014203250104890202506181446530082] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:0
push data[type=4, serial=MBCP00000011, len=500] via MB SUCCESSED, 剩余:31
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7880666, L_21757414, [FLASH]S_0, M_0, L_371907200
Total consumption of ink on startup：1_[C], [PRINT]S_14699, M_6744888, L_13465571, [FLASH]S_0, M_0, L_371907200
Total consumption of ink on startup：2_[M], [PRINT]S_14274, M_6727491, L_13464210, [FLASH]S_0, M_0, L_371907200
Total consumption of ink on startup：3_[Y], [PRINT]S_14235, M_6734412, L_13475264, [FLASH]S_0, M_0, L_371907200
iot_status:3
HTTP丢包率：11/11
data[type=512,serial=0014203250104890202506181448200088] 入待发送队列
iot_status:3
iot_status:3
wait data[type=4, serial=0014203250104890202506181446530082] 响应超时(20), 重入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7880906, L_22573174, [FLASH]S_0, M_0, L_371907200
Total consumption of ink on startup：1_[C], [PRINT]S_6773526, M_6746328, L_14280131, [FLASH]S_0, M_0, L_371907200
Total consumption of ink on startup：2_[M], [PRINT]S_49341841, M_34407647, L_14922913, [FLASH]S_0, M_0, L_371907200
Total consumption of ink on startup：3_[Y], [PRINT]S_15631993, M_6734652, L_14291024, [FLASH]S_0, M_0, L_371907200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181448410090] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：11/11
data[type=512,serial=0014203250104890202506181449210091] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181451110000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7880906, L_22573174, [FLASH]S_0, M_0, L_371907200
Total consumption of ink on startup：1_[C], [PRINT]S_6773526, M_6746328, L_14280131, [FLASH]S_0, M_0, L_371907200
Total consumption of ink on startup：2_[M], [PRINT]S_49341841, M_34407647, L_14922913, [FLASH]S_0, M_0, L_371907200
Total consumption of ink on startup：3_[Y], [PRINT]S_15631993, M_6734652, L_14291024, [FLASH]S_0, M_0, L_371907200
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181452120001] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=391] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181452120001] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181453130002] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000002, len=391] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250104890202506181453130002] 响应超时(20), 丢弃
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181454140003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181455150004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181456160005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_15034, M_7880906, L_22573174, [FLASH]S_0, M_0, L_384720000
Total consumption of ink on startup：1_[C], [PRINT]S_6773526, M_6746328, L_14280131, [FLASH]S_0, M_0, L_384720000
Total consumption of ink on startup：2_[M], [PRINT]S_49341841, M_34407647, L_14922913, [FLASH]S_0, M_0, L_384720000
Total consumption of ink on startup：3_[Y], [PRINT]S_15631993, M_6734652, L_14291024, [FLASH]S_0, M_0, L_384720000
Total consumption of ink on startup：0_[K], [PRINT]S_16102, M_7882002, L_22927021, [FLASH]S_0, M_0, L_384720000
Total consumption of ink on startup：1_[C], [PRINT]S_6774590, M_6747568, L_14626307, [FLASH]S_0, M_0, L_384720000
Total consumption of ink on startup：2_[M], [PRINT]S_49342905, M_34408903, L_15269073, [FLASH]S_0, M_0, L_384720000
Total consumption of ink on startup：3_[Y], [PRINT]S_15633057, M_6735748, L_14637344, [FLASH]S_0, M_0, L_384720000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181456450007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181457170008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181458180009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181459190010] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_16102, M_7882002, L_22927021, [FLASH]S_0, M_0, L_397545600
Total consumption of ink on startup：1_[C], [PRINT]S_6774590, M_6747568, L_14626307, [FLASH]S_0, M_0, L_397545600
Total consumption of ink on startup：2_[M], [PRINT]S_49342905, M_34408903, L_15269073, [FLASH]S_0, M_0, L_397545600
Total consumption of ink on startup：3_[Y], [PRINT]S_15633057, M_6735748, L_14637344, [FLASH]S_0, M_0, L_397545600
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_16102, M_7896369, L_23676752, [FLASH]S_0, M_0, L_397545600
Total consumption of ink on startup：1_[C], [PRINT]S_6774590, M_6748360, L_15115115, [FLASH]S_0, M_0, L_397545600
Total consumption of ink on startup：2_[M], [PRINT]S_49342905, M_34409767, L_15757809, [FLASH]S_0, M_0, L_397545600
Total consumption of ink on startup：3_[Y], [PRINT]S_15633057, M_6735892, L_15126800, [FLASH]S_0, M_0, L_397545600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181459470011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181500200012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_16102, M_7896369, L_23676752, [FLASH]S_0, M_0, L_410374400
Total consumption of ink on startup：1_[C], [PRINT]S_6774590, M_6748360, L_15115115, [FLASH]S_0, M_0, L_410374400
Total consumption of ink on startup：2_[M], [PRINT]S_49342905, M_34409767, L_15757809, [FLASH]S_0, M_0, L_410374400
Total consumption of ink on startup：3_[Y], [PRINT]S_15633057, M_6735892, L_15126800, [FLASH]S_0, M_0, L_410374400
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_16102, M_7896609, L_24492512, [FLASH]S_0, M_0, L_410374400
Total consumption of ink on startup：1_[C], [PRINT]S_13533417, M_6749800, L_15929675, [FLASH]S_0, M_0, L_410374400
Total consumption of ink on startup：2_[M], [PRINT]S_98670472, M_62089923, L_17216512, [FLASH]S_0, M_0, L_410374400
Total consumption of ink on startup：3_[Y], [PRINT]S_31250815, M_6736132, L_15942560, [FLASH]S_0, M_0, L_410374400
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181500580014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181501210015] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_16102, M_7896609, L_24492512, [FLASH]S_0, M_0, L_423196800
Total consumption of ink on startup：1_[C], [PRINT]S_13533417, M_6749800, L_15929675, [FLASH]S_0, M_0, L_423196800
Total consumption of ink on startup：2_[M], [PRINT]S_98670472, M_62089923, L_17216512, [FLASH]S_0, M_0, L_423196800
Total consumption of ink on startup：3_[Y], [PRINT]S_31250815, M_6736132, L_15942560, [FLASH]S_0, M_0, L_423196800
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_465056, M_11698903, L_25584477, [FLASH]S_0, M_0, L_423196800
Total consumption of ink on startup：1_[C], [PRINT]S_13982362, M_8335712, L_16971453, [FLASH]S_0, M_0, L_423196800
Total consumption of ink on startup：2_[M], [PRINT]S_99119417, M_63675762, L_18258267, [FLASH]S_0, M_0, L_423196800
Total consumption of ink on startup：3_[Y], [PRINT]S_31699748, M_8321789, L_16984562, [FLASH]S_0, M_0, L_423196800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181502020016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181502220017] 入待发送队列
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181520580000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_465056, M_11698903, L_25584477, [FLASH]S_0, M_0, L_423196800
Total consumption of ink on startup：1_[C], [PRINT]S_13982362, M_8335712, L_16971453, [FLASH]S_0, M_0, L_423196800
Total consumption of ink on startup：2_[M], [PRINT]S_99119417, M_63675762, L_18258267, [FLASH]S_0, M_0, L_423196800
Total consumption of ink on startup：3_[Y], [PRINT]S_31699748, M_8321789, L_16984562, [FLASH]S_0, M_0, L_423196800
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181521590001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181523000002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=391] via MB SUCCESSED, 剩余:0
wait data[type=512, serial=0014203250104890202506181523000002] 响应超时(20), 丢弃
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181524080003] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000002, len=391] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_465056, M_11698903, L_25584477, [FLASH]S_0, M_0, L_436025600
Total consumption of ink on startup：1_[C], [PRINT]S_13982362, M_8335712, L_16971453, [FLASH]S_0, M_0, L_436025600
Total consumption of ink on startup：2_[M], [PRINT]S_99119417, M_63675762, L_18258267, [FLASH]S_0, M_0, L_436025600
Total consumption of ink on startup：3_[Y], [PRINT]S_31699748, M_8321789, L_16984562, [FLASH]S_0, M_0, L_436025600
wait data[type=512, serial=0014203250104890202506181524080003] 响应超时(20), 丢弃
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_465056, M_11699143, L_26400237, [FLASH]S_0, M_0, L_436025600
Total consumption of ink on startup：1_[C], [PRINT]S_20741189, M_8337152, L_17786013, [FLASH]S_0, M_0, L_436025600
Total consumption of ink on startup：2_[M], [PRINT]S_148446984, M_91355918, L_19716970, [FLASH]S_0, M_0, L_436025600
Total consumption of ink on startup：3_[Y], [PRINT]S_47317506, M_8322029, L_17800322, [FLASH]S_0, M_0, L_436025600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181524540005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181525090006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_465056, M_11699143, L_26400237, [FLASH]S_0, M_0, L_448835200
Total consumption of ink on startup：1_[C], [PRINT]S_20741189, M_8337152, L_17786013, [FLASH]S_0, M_0, L_448835200
Total consumption of ink on startup：2_[M], [PRINT]S_148446984, M_91355918, L_19716970, [FLASH]S_0, M_0, L_448835200
Total consumption of ink on startup：3_[Y], [PRINT]S_47317506, M_8322029, L_17800322, [FLASH]S_0, M_0, L_448835200
Total consumption of ink on startup：0_[K], [PRINT]S_466124, M_11700239, L_26754095, [FLASH]S_0, M_0, L_448835200
Total consumption of ink on startup：1_[C], [PRINT]S_20742253, M_8338392, L_18132189, [FLASH]S_0, M_0, L_448835200
Total consumption of ink on startup：2_[M], [PRINT]S_148448048, M_91357174, L_20063130, [FLASH]S_0, M_0, L_448835200
Total consumption of ink on startup：3_[Y], [PRINT]S_47318570, M_8323125, L_18146642, [FLASH]S_0, M_0, L_448835200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181525310007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181526100008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181527110009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_466124, M_11700239, L_26754095, [FLASH]S_0, M_0, L_461664000
Total consumption of ink on startup：1_[C], [PRINT]S_20742253, M_8338392, L_18132189, [FLASH]S_0, M_0, L_461664000
Total consumption of ink on startup：2_[M], [PRINT]S_148448048, M_91357174, L_20063130, [FLASH]S_0, M_0, L_461664000
Total consumption of ink on startup：3_[Y], [PRINT]S_47318570, M_8323125, L_18146642, [FLASH]S_0, M_0, L_461664000
Total consumption of ink on startup：0_[K], [PRINT]S_467192, M_11701335, L_27107831, [FLASH]S_0, M_0, L_461664000
Total consumption of ink on startup：1_[C], [PRINT]S_20743317, M_8339632, L_18478365, [FLASH]S_0, M_0, L_461664000
Total consumption of ink on startup：2_[M], [PRINT]S_148449112, M_91358430, L_20409290, [FLASH]S_0, M_0, L_461664000
Total consumption of ink on startup：3_[Y], [PRINT]S_47319634, M_8324221, L_18492962, [FLASH]S_0, M_0, L_461664000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181527330010] 入待发送队列
iot_status:0
push data[type=2, serial=MBCP00000003, len=951] via MB SUCCESSED, 剩余:4
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_467192, M_11701335, L_27107831, [FLASH]S_0, M_0, L_474492800
Total consumption of ink on startup：1_[C], [PRINT]S_20743317, M_8339632, L_18478365, [FLASH]S_0, M_0, L_474492800
Total consumption of ink on startup：2_[M], [PRINT]S_148449112, M_91358430, L_20409290, [FLASH]S_0, M_0, L_474492800
Total consumption of ink on startup：3_[Y], [PRINT]S_47319634, M_8324221, L_18492962, [FLASH]S_0, M_0, L_474492800
wait data[type=2, serial=0014203250104890202506181527330010] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181528120011] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_467192, M_11701575, L_27923591, [FLASH]S_0, M_0, L_474492800
Total consumption of ink on startup：1_[C], [PRINT]S_27502144, M_8341072, L_19292925, [FLASH]S_0, M_0, L_474492800
Total consumption of ink on startup：2_[M], [PRINT]S_197776679, M_119038586, L_21867993, [FLASH]S_0, M_0, L_474492800
Total consumption of ink on startup：3_[Y], [PRINT]S_62937392, M_8324461, L_19308722, [FLASH]S_0, M_0, L_474492800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181528320012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250104890202506181529130013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000004, len=391] via MB SUCCESSED, 剩余:5
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181530140014] 入待发送队列
wait data[type=512, serial=0014203250104890202506181529130013] 响应超时(20), 丢弃
push data[type=512, serial=MBCP00000005, len=391] via MB FAILED, 剩余:5
iot_status:0
push data[type=2, serial=MBCP00000006, len=958] via MB FAILED, 剩余:4
data[type=2, serial=0014203250104890202506181528320012] 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250104890202506181531080015] 入待发送队列
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181531150016] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_467192, M_11701575, L_27923591, [FLASH]S_0, M_0, L_487312000
Total consumption of ink on startup：1_[C], [PRINT]S_27502144, M_8341072, L_19292925, [FLASH]S_0, M_0, L_487312000
Total consumption of ink on startup：2_[M], [PRINT]S_197776679, M_119038586, L_21867993, [FLASH]S_0, M_0, L_487312000
Total consumption of ink on startup：3_[Y], [PRINT]S_62937392, M_8324461, L_19308722, [FLASH]S_0, M_0, L_487312000
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181531330018] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_467192, M_11701607, L_28032359, [FLASH]S_0, M_0, L_487312000
Total consumption of ink on startup：1_[C], [PRINT]S_27799117, M_8341264, L_19401533, [FLASH]S_0, M_0, L_487312000
Total consumption of ink on startup：2_[M], [PRINT]S_198519828, M_119360381, L_21984061, [FLASH]S_0, M_0, L_487312000
Total consumption of ink on startup：3_[Y], [PRINT]S_63333064, M_8324493, L_19417490, [FLASH]S_0, M_0, L_487312000
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_467192, M_11701607, L_28032359, [FLASH]S_0, M_0, L_500150400
Total consumption of ink on startup：1_[C], [PRINT]S_27799117, M_8341264, L_19401533, [FLASH]S_0, M_0, L_500150400
Total consumption of ink on startup：2_[M], [PRINT]S_198519828, M_119360381, L_21984061, [FLASH]S_0, M_0, L_500150400
Total consumption of ink on startup：3_[Y], [PRINT]S_63333064, M_8324493, L_19417490, [FLASH]S_0, M_0, L_500150400
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181532160019] 入待发送队列
iot_status:3
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181532210020] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=0014203250104890202506181532210021] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_467192, M_11701783, L_28630583, [FLASH]S_0, M_0, L_500150400
Total consumption of ink on startup：1_[C], [PRINT]S_33716813, M_8342320, L_19998877, [FLASH]S_0, M_0, L_500150400
Total consumption of ink on startup：2_[M], [PRINT]S_240868241, M_143653841, L_23146678, [FLASH]S_0, M_0, L_500150400
Total consumption of ink on startup：3_[Y], [PRINT]S_77028496, M_8324669, L_20015714, [FLASH]S_0, M_0, L_500150400
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_467192, M_11701783, L_28630583, [FLASH]S_0, M_0, L_512966400
Total consumption of ink on startup：1_[C], [PRINT]S_33716813, M_8342320, L_19998877, [FLASH]S_0, M_0, L_512966400
Total consumption of ink on startup：2_[M], [PRINT]S_240868241, M_143653841, L_23146678, [FLASH]S_0, M_0, L_512966400
Total consumption of ink on startup：3_[Y], [PRINT]S_77028496, M_8324669, L_20015714, [FLASH]S_0, M_0, L_512966400
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250104890202506181533170022] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_467192, M_11702023, L_29446343, [FLASH]S_0, M_0, L_512966400
Total consumption of ink on startup：1_[C], [PRINT]S_40475640, M_8343760, L_20813437, [FLASH]S_0, M_0, L_512966400
Total consumption of ink on startup：2_[M], [PRINT]S_290195808, M_171333997, L_24605381, [FLASH]S_0, M_0, L_512966400
Total consumption of ink on startup：3_[Y], [PRINT]S_92646254, M_8324909, L_20831474, [FLASH]S_0, M_0, L_512966400
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181546120000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_916146, M_15504317, L_30538339, [FLASH]S_0, M_0, L_525795200
Total consumption of ink on startup：1_[C], [PRINT]S_40924585, M_9929672, L_21855215, [FLASH]S_0, M_0, L_525795200
Total consumption of ink on startup：2_[M], [PRINT]S_290644753, M_172919836, L_25647136, [FLASH]S_0, M_0, L_525795200
Total consumption of ink on startup：3_[Y], [PRINT]S_93095187, M_9910566, L_21873476, [FLASH]S_0, M_0, L_525795200
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_916146, M_15504317, L_30538339, [FLASH]S_0, M_0, L_538620800
Total consumption of ink on startup：1_[C], [PRINT]S_40924585, M_9929672, L_21855215, [FLASH]S_0, M_0, L_538620800
Total consumption of ink on startup：2_[M], [PRINT]S_290644753, M_172919836, L_25647136, [FLASH]S_0, M_0, L_538620800
Total consumption of ink on startup：3_[Y], [PRINT]S_93095187, M_9910566, L_21873476, [FLASH]S_0, M_0, L_538620800
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181547130001] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_916146, M_15504557, L_31354099, [FLASH]S_0, M_0, L_538620800
Total consumption of ink on startup：1_[C], [PRINT]S_47683412, M_9931112, L_22669775, [FLASH]S_0, M_0, L_538620800
Total consumption of ink on startup：2_[M], [PRINT]S_339972320, M_200599992, L_27105839, [FLASH]S_0, M_0, L_538620800
Total consumption of ink on startup：3_[Y], [PRINT]S_108712945, M_9910806, L_22689236, [FLASH]S_0, M_0, L_538620800
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181547150002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181548140004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_916146, M_15504557, L_31354099, [FLASH]S_0, M_0, L_551449600
Total consumption of ink on startup：1_[C], [PRINT]S_47683412, M_9931112, L_22669775, [FLASH]S_0, M_0, L_551449600
Total consumption of ink on startup：2_[M], [PRINT]S_339972320, M_200599992, L_27105839, [FLASH]S_0, M_0, L_551449600
Total consumption of ink on startup：3_[Y], [PRINT]S_108712945, M_9910806, L_22689236, [FLASH]S_0, M_0, L_551449600
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250104890202506181549150005] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181549400007] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_916146, M_15504749, L_32006707, [FLASH]S_0, M_0, L_551449600
Total consumption of ink on startup：1_[C], [PRINT]S_54024540, M_9932264, L_23321423, [FLASH]S_0, M_0, L_551449600
Total consumption of ink on startup：2_[M], [PRINT]S_386141598, M_226723527, L_28365674, [FLASH]S_0, M_0, L_551449600
Total consumption of ink on startup：3_[Y], [PRINT]S_123417342, M_9910998, L_23341844, [FLASH]S_0, M_0, L_551449600
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000001, len=767] via MB SUCCESSED, 剩余:4
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181550160008] 入待发送队列
iot_status:3
iot_status:3
wait data[type=2, serial=0014203250104890202506181549400007] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250104890202506181551000009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181551170010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181552180011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_916146, M_15504749, L_32006707, [FLASH]S_0, M_0, L_564281600
Total consumption of ink on startup：1_[C], [PRINT]S_54024540, M_9932264, L_23321423, [FLASH]S_0, M_0, L_564281600
Total consumption of ink on startup：2_[M], [PRINT]S_386141598, M_226723527, L_28365674, [FLASH]S_0, M_0, L_564281600
Total consumption of ink on startup：3_[Y], [PRINT]S_123417342, M_9910998, L_23341844, [FLASH]S_0, M_0, L_564281600
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181553190012] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181553460013] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181554200014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5999, M_9310, L_6009, [FLASH]S_0, M_0, L_12825600
Total consumption of ink on startup：1_[C], [PRINT]S_5880, M_9233, L_6016, [FLASH]S_0, M_0, L_12825600
Total consumption of ink on startup：2_[M], [PRINT]S_5821, M_9288, L_5950, [FLASH]S_0, M_0, L_12825600
Total consumption of ink on startup：3_[Y], [PRINT]S_5829, M_9328, L_5856, [FLASH]S_0, M_0, L_12825600
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181555210015] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5999, M_23677, L_755712, [FLASH]S_0, M_0, L_12825600
Total consumption of ink on startup：1_[C], [PRINT]S_5880, M_10025, L_494824, [FLASH]S_0, M_0, L_12825600
Total consumption of ink on startup：2_[M], [PRINT]S_5821, M_10152, L_494686, [FLASH]S_0, M_0, L_12825600
Total consumption of ink on startup：3_[Y], [PRINT]S_5829, M_9472, L_495312, [FLASH]S_0, M_0, L_12825600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181555300016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250104890202506181556000017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250104890202506181556220018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5999, M_23677, L_755712, [FLASH]S_0, M_0, L_25651200
Total consumption of ink on startup：1_[C], [PRINT]S_5880, M_10025, L_494824, [FLASH]S_0, M_0, L_25651200
Total consumption of ink on startup：2_[M], [PRINT]S_5821, M_10152, L_494686, [FLASH]S_0, M_0, L_25651200
Total consumption of ink on startup：3_[Y], [PRINT]S_5829, M_9472, L_495312, [FLASH]S_0, M_0, L_25651200
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5999, M_23917, L_1571472, [FLASH]S_0, M_0, L_25651200
Total consumption of ink on startup：1_[C], [PRINT]S_6764707, M_11465, L_1309384, [FLASH]S_0, M_0, L_25651200
Total consumption of ink on startup：2_[M], [PRINT]S_49333388, M_27690308, L_1953389, [FLASH]S_0, M_0, L_25651200
Total consumption of ink on startup：3_[Y], [PRINT]S_15623587, M_9712, L_1311072, [FLASH]S_0, M_0, L_25651200
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250104890202506181557020019] 入待发送队列
iot_status:3
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=0014203250104890202506181557020020] 入待发送队列
iot_status:3
iot_status:3
iot_status:0
push data[type=1, serial=MBCP00000002, len=959] via MB SUCCESSED, 剩余:10
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181557230021] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5999, M_23917, L_1571472, [FLASH]S_0, M_0, L_38473600
Total consumption of ink on startup：1_[C], [PRINT]S_6764707, M_11465, L_1309384, [FLASH]S_0, M_0, L_38473600
Total consumption of ink on startup：2_[M], [PRINT]S_49333388, M_27690308, L_1953389, [FLASH]S_0, M_0, L_38473600
Total consumption of ink on startup：3_[Y], [PRINT]S_15623587, M_9712, L_1311072, [FLASH]S_0, M_0, L_38473600
wait data[type=1, serial=0014203250104890202506181557020020] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_5999, M_24221, L_2604768, [FLASH]S_0, M_0, L_38473600
Total consumption of ink on startup：1_[C], [PRINT]S_13523534, M_13289, L_2341160, [FLASH]S_0, M_0, L_38473600
Total consumption of ink on startup：2_[M], [PRINT]S_98488920, M_55370816, L_3629340, [FLASH]S_0, M_0, L_38473600
Total consumption of ink on startup：3_[Y], [PRINT]S_31241345, M_10016, L_2344368, [FLASH]S_0, M_0, L_38473600
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=0014203250104890202506181558050022] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181558240024] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181559250025] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181600260026] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250104890202506181601100027] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181602010028] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=0014203250104890202506181603020029] 入待发送队列
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181612440000] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_7954, L_1044486, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_6767673, M_9815, L_1043153, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_49164703, M_27686984, L_1688591, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_15627010, M_9703, L_1042870, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181613450003] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181614460004] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181615470005] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181616480006] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181617490007] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181618500008] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181619510009] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181620520010] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181626440011] 入待发送队列
data[type=4,serial=00142321125841202506181626470012] 入待发送队列
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181649340000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_8258, L_2077782, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_13526500, M_11639, L_2074929, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_98320235, M_55366124, L_3365910, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_31244768, M_11375, L_2074798, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_8258, L_2077782, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_13526500, M_11639, L_2074929, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_98320235, M_55366124, L_3365910, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_31244768, M_11375, L_2074798, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_8562, L_3111078, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_20285327, M_13463, L_3106705, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_147475767, M_83045264, L_5043229, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_46862526, M_13047, L_3106726, [FLASH]S_0, M_0, L_0
iot_status:-1
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00142321125841202506181650280002] 入待发送队列
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181650350003] 入待发送队列
iot_status:-1
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_8562, L_3111078, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_20285327, M_13463, L_3106705, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_147475767, M_83045264, L_5043229, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_46862526, M_13047, L_3106726, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00142321125841202506181651260004] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_8786, L_3872454, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_26292079, M_14807, L_3866961, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_190326740, M_107580520, L_6376074, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_60723722, M_14279, L_3867094, [FLASH]S_0, M_0, L_0
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181651360005] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_8786, L_3872454, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_26292079, M_14807, L_3866961, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_190326740, M_107580520, L_6376074, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_60723722, M_14279, L_3867094, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_9090, L_4905750, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_33050906, M_16631, L_4898737, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_239482272, M_135259660, L_8053393, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_76341480, M_15951, L_4899022, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00142321125841202506181652240006] 入待发送队列
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181652370007] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181653380008] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00142321125841202506181654190009] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181654390010] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181655400011] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181656410012] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181657420013] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_9090, L_4905750, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_33050906, M_16631, L_4898737, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_239482272, M_135259660, L_8053393, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_76341480, M_15951, L_4899022, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181658430014] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_9527, M_9394, L_5939046, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_39809733, M_18455, L_5930513, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_288637804, M_162938800, L_9730712, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_91959238, M_17623, L_5930950, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00142321125841202506181658520015] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181659520016] 入待发送队列
data[type=4,serial=00142321125841202506181659530017] 入待发送队列
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181700530018] 入待发送队列
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181707240019] 入待发送队列
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181708250020] 入待发送队列
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181709260021] 入待发送队列
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181710520022] 入待发送队列
HTTP丢包率：0/0
data[type=512,serial=00142321125841202506181711530023] 入待发送队列
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
