云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191049330000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191050340001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191051350002] 入待发送队列
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191052360003] 入待发送队列
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191052360004] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191053370005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191054380006] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191055390007] 入待发送队列
iot_status:3
iot_status:3
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191055550009] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191056400010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191057050011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191057410013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191058420014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191059430015] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191100440016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191101450017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191102460018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191103470019] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191104480020] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191105490021] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191106500022] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191107510023] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000001, len=392] via MB SUCCESSED, 剩余:5
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
wait data[type=512, serial=00AF503250200216202506191107510023] 响应超时(20), 丢弃
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191108190024] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191108520025] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191109250026] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191109530027] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000002, len=392] via MB SUCCESSED, 剩余:7
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191109530027] 响应超时(20), 丢弃
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191110470029] 入待发送队列
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191110540030] 入待发送队列
iot_status:3
iot_status:3
wait data[type=2, serial=00AF503250200216202506191109250026] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191111550031] 入待发送队列
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000004, len=392] via MB SUCCESSED, 剩余:9
iot_status:3
iot_status:0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
wait data[type=512, serial=00AF503250200216202506191111550031] 响应超时(20), 丢弃
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191112360032] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191112560033] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000005, len=392] via MB SUCCESSED, 剩余:10
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
wait data[type=512, serial=00AF503250200216202506191112560033] 响应超时(20), 丢弃
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191113510034] 入待发送队列
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191113570035] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191114580036] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191115180037] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191115590038] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000006, len=392] via MB SUCCESSED, 剩余:12
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191115590038] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191117000039] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191118010040] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191119020041] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191120030042] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191121040043] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191122050044] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191123060045] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000007, len=392] via MB SUCCESSED, 剩余:12
wait data[type=512, serial=00AF503250200216202506191123060045] 响应超时(20), 丢弃
push data[type=2, serial=MBCP00000008, len=792] via MB FAILED, 剩余:11
data[type=2, serial=00AF503250200216202506191115180037] 重入待发送队列
iot_status:0
push data[type=2, serial=MBCP00000009, len=792] via MB FAILED, 剩余:11
data[type=2, serial=00AF503250200216202506191115180037] 重入待发送队列
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00AF503250200216202506191124070046] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=1,serial=00AF503250200216202506191124370048] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00AF503250200216202506191125080049] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00AF503250200216202506191126090050] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00AF503250200216202506191127100051] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000010, len=392] via MB SUCCESSED, 剩余:14
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191128110052] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191127100051] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191129120053] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191130130054] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191131140055] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191132150056] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191133160057] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191134170058] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191135180059] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000011, len=392] via MB SUCCESSED, 剩余:14
iot_status:3
iot_status:0
HTTP丢包率：9/9
data[type=512,serial=00AF503250200216202506191136190060] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
wait data[type=512, serial=00AF503250200216202506191135180059] 响应超时(20), 丢弃
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191136300062] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：9/9
data[type=512,serial=00AF503250200216202506191137200063] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:0
push data[type=512, serial=MBCP00000012, len=392] via MB SUCCESSED, 剩余:16
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191137320064] 入待发送队列
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=1,serial=00AF503250200216202506191137320065] 入待发送队列
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191137200063] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：10/10
data[type=512,serial=00AF503250200216202506191138210066] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191138540067] 入待发送队列
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=1,serial=00AF503250200216202506191138540068] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：10/10
data[type=512,serial=00AF503250200216202506191139220069] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
HTTP丢包率：10/10
data[type=512,serial=00AF503250200216202506191140230070] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191140580071] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：10/10
data[type=512,serial=00AF503250200216202506191141240072] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191142060073] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：10/10
data[type=512,serial=00AF503250200216202506191142250074] 入待发送队列
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000013, len=392] via MB SUCCESSED, 剩余:22
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191142250074] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：11/11
data[type=512,serial=00AF503250200216202506191143260075] 入待发送队列
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191424000000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191425010001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191426020002] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=392] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
wait data[type=512, serial=00AF503250200216202506191426020002] 响应超时(20), 丢弃
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191427030003] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191427060004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191428040005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000002, len=392] via MB SUCCESSED, 剩余:1
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191428040005] 响应超时(20), 丢弃
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191429050006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191430050007] 入待发送队列
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191430060008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191431070009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:0
push data[type=512, serial=MBCP00000003, len=392] via MB SUCCESSED, 剩余:2
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191431070009] 响应超时(20), 丢弃
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191432080010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191432370012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191433090013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191433440014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191434100015] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191435110016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191436120017] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191436240018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191437130019] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191437370020] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191438140021] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191438300022] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191439150023] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191440160024] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000004, len=392] via MB SUCCESSED, 剩余:8
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191440160024] 响应超时(20), 丢弃
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191441170025] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191442180026] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191443190027] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191444200028] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000005, len=392] via MB SUCCESSED, 剩余:8
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191445210029] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
wait data[type=512, serial=00AF503250200216202506191444200028] 响应超时(20), 丢弃
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191445350030] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191446220031] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191447230032] 入待发送队列
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000006, len=392] via MB SUCCESSED, 剩余:9
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191447230032] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191448240033] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191449250034] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191450260035] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000007, len=392] via MB SUCCESSED, 剩余:9
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191450260035] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00AF503250200216202506191451270036] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00AF503250200216202506191452280037] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00AF503250200216202506191453290038] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00AF503250200216202506191454300039] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000008, len=392] via MB SUCCESSED, 剩余:9
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191454300039] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191455310040] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191456320041] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00AF503250200216202506191457330042] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000009, len=392] via MB SUCCESSED, 剩余:9
iot_status:3
iot_status:3
HTTP丢包率：9/9
data[type=512,serial=00AF503250200216202506191458340043] 入待发送队列
iot_status:3
wait data[type=512, serial=00AF503250200216202506191457330042] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191459070044] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：9/9
data[type=512,serial=00AF503250200216202506191459350045] 入待发送队列
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
iot_status:3
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191503300000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191504310001] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191504370002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191505320003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191506330004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191507340005] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191507460006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000001, len=792] via MB SUCCESSED, 剩余:2
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191508350007] 入待发送队列
iot_status:3
iot_status:3
wait data[type=2, serial=00AF503250200216202506191507460006] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191509360008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191510370009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191511380010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191512110011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191512390012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191522250000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191523260001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191524270002] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191524290003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000001, len=792] via MB SUCCESSED, 剩余:1
iot_status:3
iot_status:3
iot_status:3
wait data[type=2, serial=00AF503250200216202506191524290003] 响应超时(20), 重入待发送队列
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191525280004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
iot_status:3
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191553100000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191554110001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191555120002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=392] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191555120002] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191556130003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191557140004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191558150005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191559160006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191600170007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191601180008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191602190009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191603200010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191604210011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191605220012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191606230013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191607240014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191608250015] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191613440016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191614450017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191615460018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191616470019] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191617480020] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000002, len=392] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191617480020] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191618490021] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191619500022] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191620510023] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191621520024] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191622530025] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191623540026] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191624550027] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191625560028] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191626570029] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191627580030] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191628590031] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191630000032] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191631010033] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191632020034] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191633030035] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191634040036] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191635000037] 入待发送队列
iot_status:0
push data[type=2, serial=MBCP00000003, len=758] via MB SUCCESSED, 剩余:1
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191635050038] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
wait data[type=2, serial=00AF503250200216202506191635000037] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191636060039] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191636320040] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191637070041] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191638080042] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191638280043] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191639090044] 入待发送队列
iot_status:3
iot_status:3
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191639230045] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000004, len=780] via MB SUCCESSED, 剩余:4
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191640100046] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
wait data[type=2, serial=00AF503250200216202506191639230045] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191641110047] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191641380048] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191642120049] 入待发送队列
iot_status:0
push data[type=512, serial=MBCP00000005, len=392] via MB SUCCESSED, 剩余:5
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191642120049] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191643130050] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191643550051] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191644140052] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191645150053] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191646160054] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191647170055] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191648180056] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191649190057] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191650190058] 入待发送队列
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=1,serial=00AF503250200216202506191650190059] 入待发送队列
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191650200060] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000006, len=392] via MB SUCCESSED, 剩余:8
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191650200060] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191651210061] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191652220062] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191653230063] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191654240064] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191655250065] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191656260066] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191657270067] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191658280068] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191659290069] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191700300070] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191701310071] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191702320072] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191703330073] 入待发送队列
iot_status:3
data[type=4,serial=00AF503250200216202506191703440074] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191717120075] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191718130076] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191719140077] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191720150078] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191721160079] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191722170080] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191723180081] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191724190082] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191725200083] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191726210084] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00AF503250200216202506191727220085] 入待发送队列
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191730110000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191731120001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191732130002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191733140003] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=392] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191733140003] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191734150004] 入待发送队列
push data[type=512, serial=MBCP00000002, len=392] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191734150004] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191735160005] 入待发送队列
push data[type=512, serial=MBCP00000003, len=392] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191735160005] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191736170006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=1,serial=00AF503250200216202506191736590007] 入待发送队列
iot_status:3
iot_status:0
push data[type=1, serial=MBCP00000004, len=812] via MB SUCCESSED, 剩余:1
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191737180008] 入待发送队列
iot_status:3
iot_status:3
wait data[type=1, serial=00AF503250200216202506191736590007] 响应超时(20), 丢弃
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191737320009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191738190010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191739200011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191739590012] 入待发送队列
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=1,serial=00AF503250200216202506191739590013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191740210014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191741220015] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191742230016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191743240017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191744250018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191745260019] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191746270020] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191747280021] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191748290022] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191749300023] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191750310024] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191751320025] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191752330026] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191753340027] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191819300028] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191820310029] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191821320030] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191822330031] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191823340032] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191824350033] 入待发送队列
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191824400034] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191838330000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191839340001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191840350002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191841360003] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=392] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191841360003] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00AF503250200216202506191842370004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000002, len=392] via MB SUCCESSED, 剩余:0
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00AF503250200216202506191843380005] 入待发送队列
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=1,serial=00AF503250200216202506191843390006] 入待发送队列
wait data[type=512, serial=00AF503250200216202506191842370004] 响应超时(20), 丢弃
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191843460007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000003, len=799] via MB SUCCESSED, 剩余:2
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191844390008] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191844460009] 入待发送队列
iot_status:3
wait data[type=2, serial=00AF503250200216202506191843460007] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=00AF503250200216202506191845400010] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000004, len=392] via MB SUCCESSED, 剩余:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191845400010] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191846410011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=00AF503250200216202506191847420012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000005, len=392] via MB SUCCESSED, 剩余:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00AF503250200216202506191847420012] 响应超时(20), 丢弃
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191848430013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191849440014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=1,serial=00AF503250200216202506191850320015] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
墨点大小,SMB:3.500000-7.000000-11.000000
data[type=2,serial=00AF503250200216202506191850390016] 入待发送队列
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191850450017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191851460018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191852470019] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191853480020] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191854490021] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00AF503250200216202506191855500022] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191927520000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191928530001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191929540002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191930550003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191931560004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191932570005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191933580006] 入待发送队列
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191934480000] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：8_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00AF503250200216202506191935490001] 入待发送队列
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
