云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061019210000] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_2191091, M_786768, L_45414376, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1903922, M_744186, L_40312066, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1911476, M_742433, L_40311678, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1914297, M_749012, L_40335716, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1064, M_1064, L_131968, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1064, M_1064, L_131960, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061020220001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061021230002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061022240003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061023250004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061024260005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061025270006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：4_[Lc], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：5_[Lm], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：6_[Lk], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：7_[Llk], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：11_[-W], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202506061315570000] 入待发送队列
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202506061315570001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202506061315570002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061315570000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
iot_status:0
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061315570002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061315570001,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202506061316580003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061316580003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202506061317590004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061317590004,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202506061319000005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061319000005,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202506061320010006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061320010006,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
data[type=4,serial=006EA1B2C3D4E5202506061320480007] 入待发送队列
push data[type=4, serial=MBCP00000008, len=419] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
运行状态数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061320480007,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202506061321020008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061321020008,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/9
data[type=512,serial=006EA1B2C3D4E5202506061322030009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061322030009,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/10
data[type=512,serial=006EA1B2C3D4E5202506061323040010] 入待发送队列
push data[type=512, serial=MBCP00000011, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061323040010,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/11
data[type=512,serial=006EA1B2C3D4E5202506061324050011] 入待发送队列
push data[type=512, serial=MBCP00000012, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061324050011,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/12
data[type=512,serial=006EA1B2C3D4E5202506061325060012] 入待发送队列
push data[type=512, serial=MBCP00000013, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061325060012,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/13
data[type=512,serial=006EA1B2C3D4E5202506061326070013] 入待发送队列
push data[type=512, serial=MBCP00000014, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061326070013,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/14
data[type=512,serial=006EA1B2C3D4E5202506061327080014] 入待发送队列
push data[type=512, serial=MBCP00000015, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061327080014,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/15
data[type=512,serial=006EA1B2C3D4E5202506061328090015] 入待发送队列
push data[type=512, serial=MBCP00000016, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061328090015,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/16
data[type=512,serial=006EA1B2C3D4E5202506061329100016] 入待发送队列
push data[type=512, serial=MBCP00000017, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061329100016,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/17
data[type=512,serial=006EA1B2C3D4E5202506061330110017] 入待发送队列
push data[type=512, serial=MBCP00000018, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061330110017,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/18
data[type=512,serial=006EA1B2C3D4E5202506061331120018] 入待发送队列
push data[type=512, serial=MBCP00000019, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061331120018,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/19
data[type=512,serial=006EA1B2C3D4E5202506061332130019] 入待发送队列
push data[type=512, serial=MBCP00000020, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061332130019,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/20
data[type=512,serial=006EA1B2C3D4E5202506061333140020] 入待发送队列
push data[type=512, serial=MBCP00000021, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061333140020,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/21
data[type=512,serial=006EA1B2C3D4E5202506061334150021] 入待发送队列
push data[type=512, serial=MBCP00000022, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061334150021,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/22
data[type=512,serial=006EA1B2C3D4E5202506061335160022] 入待发送队列
push data[type=512, serial=MBCP00000023, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061335160022,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/23
data[type=512,serial=006EA1B2C3D4E5202506061336170023] 入待发送队列
push data[type=512, serial=MBCP00000024, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061336170023,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/24
data[type=512,serial=006EA1B2C3D4E5202506061337180024] 入待发送队列
push data[type=512, serial=MBCP00000025, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061337180024,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/25
data[type=512,serial=006EA1B2C3D4E5202506061338190025] 入待发送队列
push data[type=512, serial=MBCP00000026, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061338190025,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/26
data[type=512,serial=006EA1B2C3D4E5202506061339200026] 入待发送队列
push data[type=512, serial=MBCP00000027, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061339200026,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/27
data[type=512,serial=006EA1B2C3D4E5202506061340210027] 入待发送队列
push data[type=512, serial=MBCP00000028, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061340210027,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/28
data[type=512,serial=006EA1B2C3D4E5202506061341220028] 入待发送队列
push data[type=512, serial=MBCP00000029, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061341220028,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/29
data[type=512,serial=006EA1B2C3D4E5202506061342230029] 入待发送队列
push data[type=512, serial=MBCP00000030, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061342230029,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/30
data[type=512,serial=006EA1B2C3D4E5202506061343240030] 入待发送队列
push data[type=512, serial=MBCP00000031, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061343240030,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/31
data[type=512,serial=006EA1B2C3D4E5202506061344250031] 入待发送队列
push data[type=512, serial=MBCP00000032, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061344250031,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/32
data[type=512,serial=006EA1B2C3D4E5202506061345260032] 入待发送队列
push data[type=512, serial=MBCP00000033, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061345260032,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：4_[Lc], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：5_[Lm], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：6_[Lk], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：7_[Llk], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：11_[-W], [PRINT]S_0, M_0, L_0, [FLASH]S_480, M_480, L_480
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/33
data[type=512,serial=006EA1B2C3D4E5202506061346270033] 入待发送队列
push data[type=512, serial=MBCP00000034, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061346270033,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/34
data[type=512,serial=006EA1B2C3D4E5202506061347280034] 入待发送队列
push data[type=512, serial=MBCP00000035, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061347280034,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/35
data[type=512,serial=006EA1B2C3D4E5202506061348290035] 入待发送队列
push data[type=512, serial=MBCP00000036, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061348290035,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/36
data[type=512,serial=006EA1B2C3D4E5202506061349300036] 入待发送队列
push data[type=512, serial=MBCP00000037, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061349300036,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/37
data[type=512,serial=006EA1B2C3D4E5202506061350310037] 入待发送队列
push data[type=512, serial=MBCP00000038, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061350310037,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/38
data[type=512,serial=006EA1B2C3D4E5202506061351320038] 入待发送队列
push data[type=512, serial=MBCP00000039, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061351320038,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/39
data[type=512,serial=006EA1B2C3D4E5202506061352330039] 入待发送队列
push data[type=512, serial=MBCP00000040, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061352330039,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/40
data[type=512,serial=006EA1B2C3D4E5202506061353340040] 入待发送队列
RECV data from IOT, len=532
push data[type=512, serial=MBCP00000041, len=396] via MB SUCCESSED, 剩余:0
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061353340040,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/41
data[type=512,serial=006EA1B2C3D4E5202506061354350041] 入待发送队列
push data[type=512, serial=MBCP00000042, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061354350041,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061435370000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_266, M_266, L_41786, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_532, M_532, L_65984, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_532, M_532, L_65980, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_399, M_399, L_62653, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_399, M_399, L_49488, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_399, M_399, L_49488, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_399, M_399, L_49488, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_798, M_798, L_98976, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_798, M_798, L_98970, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_399, M_399, L_62653, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_399, M_399, L_49488, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_399, M_399, L_49488, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_399, M_399, L_49488, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_798, M_798, L_98976, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_798, M_798, L_98970, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061436150001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061436380002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061437390003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061438400004] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061439410005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=00D2203241205737202506061440420006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=392] via MB SUCCESSED, 剩余:1
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061440420006] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=00D2203241205737202506061441430007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000002, len=392] via MB SUCCESSED, 剩余:1
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061441430007] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061442440008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_532, M_532, L_83521, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_532, M_532, L_65984, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_532, M_532, L_65984, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_532, M_532, L_65984, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1064, M_1064, L_131968, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1064, M_1064, L_131960, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_532, M_532, L_83521, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_532, M_532, L_65984, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_532, M_532, L_65984, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_532, M_532, L_65984, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1064, M_1064, L_131968, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1064, M_1064, L_131960, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061443170009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061443450010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061444460011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061445470012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061446480013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061447490014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061448500015] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061449510016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_665, M_665, L_104413, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_665, M_665, L_82480, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_665, M_665, L_82480, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_665, M_665, L_82480, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1330, M_1330, L_164960, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1330, M_1330, L_164950, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_665, M_665, L_104413, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_665, M_665, L_82480, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_665, M_665, L_82480, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_665, M_665, L_82480, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1330, M_1330, L_164960, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1330, M_1330, L_164950, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061450140017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061450520018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061451530019] 入待发送队列
data[type=4,serial=00D2203241205737202506061451550020] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061452540021] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061453550022] 入待发送队列
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061454560023] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061455570024] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061456580025] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061457590026] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061459000027] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061500010028] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061501020029] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061502030030] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061503040031] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061504050032] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061505060033] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061506070034] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061507080035] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=00D2203241205737202506061508090036] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000003, len=392] via MB SUCCESSED, 剩余:4
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061508090036] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=4, serial=MBCP00000004, len=424] via MB SUCCESSED, 剩余:3
HTTP丢包率：4/4
data[type=512,serial=00D2203241205737202506061509100037] 入待发送队列
iot_status:3
iot_status:3
iot_status:0
wait data[type=4, serial=00D2203241205737202506061451550020] 响应超时(20), 重入待发送队列
push data[type=4, serial=MBCP00000005, len=424] via MB SUCCESSED, 剩余:4
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_798, M_798, L_125261, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_798, M_798, L_98976, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_798, M_798, L_98976, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_798, M_798, L_98976, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1596, M_1596, L_197952, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1596, M_1596, L_197940, [FLASH]S_0, M_0, L_0
wait data[type=4, serial=00D2203241205737202506061451550020] 响应超时(20), 重入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_798, M_798, L_125261, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_798, M_798, L_98976, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_798, M_798, L_98976, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_798, M_798, L_98976, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1596, M_1596, L_197952, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1596, M_1596, L_197940, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061509430038] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00D2203241205737202506061510110039] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：5/5
data[type=512,serial=00D2203241205737202506061511120040] 入待发送队列
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000006, len=392] via MB SUCCESSED, 剩余:5
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061511120040] 响应超时(20), 丢弃
Total consumption of ink on startup：0_[K], [PRINT]S_931, M_931, L_145961, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_931, M_931, L_115472, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_931, M_931, L_115472, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_931, M_931, L_115472, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1862, M_1862, L_230944, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1862, M_1862, L_230930, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_931, M_931, L_145961, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_931, M_931, L_115472, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_931, M_931, L_115472, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_931, M_931, L_115472, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1862, M_1862, L_230944, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1862, M_1862, L_230930, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061511590041] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061512130042] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061513140043] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061514150044] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061515160045] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061519370046] 入待发送队列
data[type=4,serial=00D2203241205737202506061519410047] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061520380048] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061521390049] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061522400050] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_133, M_133, L_20901, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_133, M_133, L_16496, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_133, M_133, L_16496, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_133, M_133, L_16496, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_266, M_266, L_32990, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_133, M_133, L_20901, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_133, M_133, L_16496, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_133, M_133, L_16496, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_133, M_133, L_16496, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_266, M_266, L_32990, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061523180051] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061523410052] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_266, M_266, L_41789, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_532, M_532, L_65984, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_532, M_532, L_65980, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_266, M_266, L_41789, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_266, M_266, L_32992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_532, M_532, L_65984, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_532, M_532, L_65980, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061524240053] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=00D2203241205737202506061524410054] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061524420055] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061525430056] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061526440057] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061527450058] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061528460059] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061543130060] 入待发送队列
data[type=4,serial=00D2203241205737202506061543130061] 入待发送队列
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061544140062] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061545150063] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061546160064] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：6/6
data[type=512,serial=00D2203241205737202506061547170065] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000007, len=392] via MB SUCCESSED, 剩余:11
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061547170065] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00D2203241205737202506061548180066] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00D2203241205737202506061549190067] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00D2203241205737202506061550200068] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00D2203241205737202506061551210069] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00D2203241205737202506061552220070] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：7/7
data[type=512,serial=00D2203241205737202506061553230071] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000008, len=392] via MB SUCCESSED, 剩余:11
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061553230071] 响应超时(20), 丢弃
HTTP丢包率：8/8
data[type=512,serial=00D2203241205737202506061554240072] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00D2203241205737202506061555250073] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00D2203241205737202506061556260074] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00D2203241205737202506061557270075] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：8/8
data[type=512,serial=00D2203241205737202506061558280076] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000009, len=392] via MB SUCCESSED, 剩余:11
HTTP丢包率：9/9
data[type=512,serial=00D2203241205737202506061559290077] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061558280076] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：9/9
data[type=512,serial=00D2203241205737202506061600300078] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：9/9
data[type=512,serial=00D2203241205737202506061601310079] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：9/9
data[type=512,serial=00D2203241205737202506061602320080] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_931, M_931, L_204886328, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_931, M_931, L_199518567, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_931, M_931, L_199518567, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_931, M_931, L_199624802, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1862, M_1862, L_230944, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1862, M_1862, L_230930, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_931, M_931, L_204886328, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_931, M_931, L_199518567, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_931, M_931, L_199518567, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_931, M_931, L_199624802, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_1862, M_1862, L_230944, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_1862, M_1862, L_230930, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061603110081] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=00D2203241205737202506061603110082] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：9/9
data[type=512,serial=00D2203241205737202506061603330083] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：9/9
data[type=512,serial=00D2203241205737202506061604340084] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：9/9
data[type=512,serial=00D2203241205737202506061605350085] 入待发送队列
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000010, len=392] via MB SUCCESSED, 剩余:13
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061605350085] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：10/10
data[type=512,serial=00D2203241205737202506061606360086] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000011, len=392] via MB SUCCESSED, 剩余:13
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061606360086] 响应超时(20), 丢弃
iot_status:3
HTTP丢包率：11/11
data[type=512,serial=00D2203241205737202506061607370087] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_1064, M_1064, L_204907186, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1064, M_1064, L_199535063, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1064, M_1064, L_199535063, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1064, M_1064, L_199641298, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2128, M_2128, L_263936, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2128, M_2128, L_263920, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_1064, M_1064, L_204907186, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1064, M_1064, L_199535063, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1064, M_1064, L_199535063, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1064, M_1064, L_199641298, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2128, M_2128, L_263936, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2128, M_2128, L_263920, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061607470088] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：11/11
data[type=512,serial=00D2203241205737202506061609390090] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_1197, M_1197, L_204927992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1197, M_1197, L_199551559, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1197, M_1197, L_199551559, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1197, M_1197, L_199657794, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2394, M_2394, L_296928, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2394, M_2394, L_296910, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_1197, M_1197, L_204927992, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1197, M_1197, L_199551559, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1197, M_1197, L_199551559, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1197, M_1197, L_199657794, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2394, M_2394, L_296928, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2394, M_2394, L_296910, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061610380091] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=00D2203241205737202506061610380092] 入待发送队列
iot_status:3
HTTP丢包率：11/11
data[type=512,serial=00D2203241205737202506061610400093] 入待发送队列
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000012, len=392] via MB SUCCESSED, 剩余:16
iot_status:3
iot_status:0
iot_status:3
wait data[type=512, serial=00D2203241205737202506061610400093] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_1330, M_1330, L_204948652, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1330, M_1330, L_199568055, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1330, M_1330, L_199568055, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1330, M_1330, L_199674290, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2660, M_2660, L_329920, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2660, M_2660, L_329900, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_1330, M_1330, L_204948652, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1330, M_1330, L_199568055, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1330, M_1330, L_199568055, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1330, M_1330, L_199674290, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2660, M_2660, L_329920, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2660, M_2660, L_329900, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061611330094] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=00D2203241205737202506061611330095] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：12/12
data[type=512,serial=00D2203241205737202506061611410096] 入待发送队列
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000013, len=392] via MB SUCCESSED, 剩余:18
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=00D2203241205737202506061611410096] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_1463, M_1463, L_204969429, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1463, M_1463, L_199584551, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1463, M_1463, L_199584551, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1463, M_1463, L_199690786, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2926, M_2926, L_362912, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2926, M_2926, L_362890, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_1463, M_1463, L_204969429, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1463, M_1463, L_199584551, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1463, M_1463, L_199584551, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1463, M_1463, L_199690786, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2926, M_2926, L_362912, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2926, M_2926, L_362890, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061612380097] 入待发送队列
iot_status:3
HTTP丢包率：13/13
data[type=512,serial=00D2203241205737202506061612420098] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：13/13
data[type=512,serial=00D2203241205737202506061613430099] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_1463, M_1463, L_205164735, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1463, M_1463, L_199584551, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1463, M_1463, L_199584551, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1463, M_1463, L_199690786, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2926, M_2926, L_362912, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2926, M_2926, L_362890, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_1463, M_1463, L_205164735, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1463, M_1463, L_199584551, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1463, M_1463, L_199584551, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_1463, M_1463, L_199690786, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：9_[W], [PRINT]S_2926, M_2926, L_362912, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：10_[V], [PRINT]S_2926, M_2926, L_362890, [FLASH]S_0, M_0, L_0
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=00D2203241205737202506061614170100] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：13/13
data[type=512,serial=00D2203241205737202506061614440101] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202506061825130000] 入待发送队列
data[type=256,serial=006EA1B2C3D4E5202506061825130001] 入待发送队列
push data[type=256, serial=MBCP00000001, len=468] via MB SUCCESSED, 剩余:1
data[type=128,serial=006EA1B2C3D4E5202506061825140002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061825130001,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061825140002,提交成功(0)
push data[type=512, serial=MBCP00000003, len=386] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061825130000,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202506061826140003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061826140003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202506061827150004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202506061827150004,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
