云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507071252040000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_770, M_770, L_770
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_30, M_30, L_30
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_30, M_30, L_30
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_30, M_30, L_30
Total consumption of ink on startup：4_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507071252050001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507071252050002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071252040000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
iot_status:0
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071252050002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071252050001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
iot_status:0
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507071258330000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_1910, M_1910, L_1910
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_60, M_60, L_60
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_60, M_60, L_60
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_60, M_60, L_60
Total consumption of ink on startup：4_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_240, M_240, L_240
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
data[type=256,serial=006EA1B2C3D4E5202507071258340001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507071258340002] 入待发送队列
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071258330000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071258340002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071258340001,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507071259340003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071259340003,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202507071300350004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071300350004,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202507071301360005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071301360005,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202507071302370006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071302370006,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/7
data[type=512,serial=006EA1B2C3D4E5202507071303380007] 入待发送队列
push data[type=512, serial=MBCP00000008, len=396] via MB SUCCESSED, 剩余:0
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071303380007,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202507071304390008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071304390008,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/9
data[type=512,serial=006EA1B2C3D4E5202507071305400009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071305400009,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/10
data[type=512,serial=006EA1B2C3D4E5202507071306410010] 入待发送队列
push data[type=512, serial=MBCP00000011, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071306410010,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/11
data[type=512,serial=006EA1B2C3D4E5202507071307420011] 入待发送队列
push data[type=512, serial=MBCP00000012, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071307420011,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/12
data[type=512,serial=006EA1B2C3D4E5202507071308430012] 入待发送队列
push data[type=512, serial=MBCP00000013, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507071308430012,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
