云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261319110000] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_16806, M_16806, L_288489, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=1,serial=0014203250506810202507261319350002] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_16806, M_16806, L_288489, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_33612, M_33612, L_576905, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261319470003] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_33612, M_33612, L_576905, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_50418, M_50418, L_865391, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261320020005] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261320120006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=391] via MB SUCCESSED, 剩余:5
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261321130007] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_50418, M_50418, L_865391, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_50685, M_50684, L_929844, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_266, M_266, L_59388, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_266, M_266, L_59387, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_266, M_266, L_59387, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=1,serial=0014203250506810202507261321230009] 入待发送队列
iot_status:3
wait data[type=512, serial=0014203250506810202507261320120006] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261322140010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261326290000] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_16806, M_16806, L_288520, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261326580001] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_16806, M_16806, L_288520, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_33612, M_33612, L_576958, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261327130002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261327300003] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_33612, M_33612, L_576958, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_50418, M_50418, L_865425, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261327360004] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_50418, M_50418, L_865425, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_67224, M_67224, L_1153890, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261327530005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_67224, M_67224, L_1153890, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_84030, M_84030, L_1442405, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261328130006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261328310007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261334060000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=391] via MB SUCCESSED, 剩余:0
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261335070001] 入待发送队列
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261401590000] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261403000001] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261403270002] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261403430003] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261404010004] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261404010005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261405020006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250506810202507261405290007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=4, serial=MBCP00000001, len=654] via MB SUCCESSED, 剩余:4
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261406030008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=4, serial=0014203250506810202507261405290007] 响应超时(20), 重入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261407040009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261408050010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261409060011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261410070012] 入待发送队列
data[type=4,serial=0014203250506810202507261410290013] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261411080014] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261412090015] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261413100016] 入待发送队列
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261414110017] 入待发送队列
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261425100000] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261426110001] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_16806, M_16806, L_288547, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261426160002] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_16806, M_16806, L_288547, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_33612, M_33612, L_577041, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261426270003] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_33612, M_33612, L_577041, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_50418, M_50418, L_865564, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261426380004] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_50418, M_50418, L_865564, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_67224, M_67224, L_1154031, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261426490005] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_67224, M_67224, L_1154031, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_84030, M_84030, L_1442555, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261427000006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506810202507261427120007] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_84030, M_84030, L_1442555, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_100836, M_100836, L_1730996, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261427230008] 入待发送队列
iot_status:0
push data[type=2, serial=MBCP00000001, len=838] via MB SUCCESSED, 剩余:6
Total consumption of ink on startup：0_[K], [PRINT]S_100836, M_100836, L_1730996, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_117642, M_117642, L_2019470, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261427320009] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_117642, M_117642, L_2019470, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_134448, M_134448, L_2307926, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261427410010] 入待发送队列
iot_status:3
wait data[type=2, serial=0014203250506810202507261427230008] 响应超时(20), 重入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_134448, M_134448, L_2307926, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_151254, M_151254, L_2596383, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261427500011] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_151254, M_151254, L_2596383, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_168060, M_168060, L_2884856, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261428000012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261428130013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_168060, M_168060, L_2884856, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_201415, M_192093, L_2903592, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261428560014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250506810202507261429100015] 入待发送队列
iot_status:3
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261429140016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_201415, M_192093, L_2903592, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_218221, M_208899, L_3192087, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261430040017] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_218221, M_208899, L_3192087, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
HTTP丢包率：1/1
data[type=512,serial=0014203250506810202507261430150018] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_235027, M_225705, L_3480626, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261430160019] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_235027, M_225705, L_3480626, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_251833, M_242511, L_3769129, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261430290020] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_251833, M_242511, L_3769129, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_268639, M_259317, L_4057586, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261430380021] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
Total consumption of ink on startup：0_[K], [PRINT]S_268639, M_259317, L_4057586, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_167914, M_1664, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_494471, M_17493, L_690, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_429281, M_128674, L_44171, [FLASH]S_0, M_0, L_0
push data[type=2, serial=MBCP00000002, len=838] via MB SUCCESSED, 剩余:16
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250506810202507261431160022] 入待发送队列
iot_status:3
wait data[type=2, serial=0014203250506810202507261430380021] 响应超时(20), 重入待发送队列
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261431280023] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_777717, M_694915, L_4376245, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_1358457, M_1921, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_1354188, M_77372, L_23540, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_2099452, M_829449, L_312685, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=2, serial=MBCP00000003, len=779] via MB SUCCESSED, 剩余:17
iot_status:3
iot_status:3
iot_status:3
wait data[type=2, serial=0014203250506810202507261431280023] 响应超时(20), 重入待发送队列
HTTP丢包率：3/3
data[type=512,serial=0014203250506810202507261432170024] 入待发送队列
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：3/3
data[type=512,serial=0014203250506810202507261433180025] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261433460026] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_97151, M_138073, L_112035, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_185460, M_113, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_162560, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_165551, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:0
push data[type=2, serial=MBCP00000004, len=779] via MB SUCCESSED, 剩余:18
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250506810202507261434100027] 入待发送队列
iot_status:3
wait data[type=2, serial=0014203250506810202507261433460026] 响应超时(20), 重入待发送队列
HTTP丢包率：4/4
data[type=512,serial=0014203250506810202507261434190028] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：4/4
data[type=512,serial=0014203250506810202507261435200029] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_97151, M_138073, L_112035, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_185460, M_113, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_162560, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_165551, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506810202507261435350030] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_112005, M_153875, L_124648, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_219994, M_123, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_191994, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_194130, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:3
iot_status:3
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261518490000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_42018, M_42018, L_1105246, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261519500001] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261520510002] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_16806, M_16806, L_288403, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506917202507261521200003] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_16806, M_16806, L_288403, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_33612, M_33612, L_576853, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506917202507261521290004] 入待发送队列
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_33612, M_33612, L_576853, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：0_[K], [PRINT]S_50418, M_50418, L_865297, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506917202507261521390005] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261521520006] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_50418, M_50418, L_865297, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261522530007] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
Total consumption of ink on startup：0_[K], [PRINT]S_67100, M_68856, L_880016, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_37984, M_11, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_32345, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_31557, M_0, L_0, [FLASH]S_0, M_0, L_0
墨点大小,SMB:3.500000-5.000000-8.000000
data[type=2,serial=0014203250506917202507261523140008] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
data[type=4,serial=0014203250506917202507261523310009] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261523540010] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261524550011] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261525560012] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261526570013] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：0/0
data[type=512,serial=0014203250506917202507261527580014] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000001, len=391] via MB SUCCESSED, 剩余:5
iot_status:3
wait data[type=512, serial=0014203250506917202507261527580014] 响应超时(20), 丢弃
iot_status:3
iot_status:0
push data[type=512, serial=MBCP00000002, len=391] via MB SUCCESSED, 剩余:5
iot_status:3
iot_status:3
iot_status:3
iot_status:3
wait data[type=512, serial=0014203250506917202507261534110015] 响应超时(20), 丢弃
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250506917202507261535120016] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250506917202507261536130017] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250506917202507261537140018] 入待发送队列
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250506917202507261538150019] 入待发送队列
iot_status:3
iot_status:3
HTTP丢包率：2/2
data[type=512,serial=0014203250506917202507261544170020] 入待发送队列
data[type=4,serial=0014203250506917202507261544200021] 入待发送队列
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507261612480000] 入待发送队列
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_30, M_30, L_30
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_30, M_30, L_30
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_30, M_30, L_30
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_30, M_30, L_30
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
iot_ccid:CCID-123, imei:IMEI-123
data[type=256,serial=006EA1B2C3D4E5202507261612480001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507261612480002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261612480000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
iot_status:0
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261612480002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261612480001,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507261613490003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB FAILED, 剩余:0
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507261614400000] 入待发送队列
data[type=256,serial=006EA1B2C3D4E5202507261614400001] 入待发送队列
push data[type=256, serial=MBCP00000001, len=468] via MB SUCCESSED, 剩余:1
iot_ccid:CCID-123, imei:IMEI-123
data[type=128,serial=006EA1B2C3D4E5202507261614400002] 入待发送队列
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261614400001,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
iot_status:0
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261614400002,提交成功(0)
push data[type=512, serial=MBCP00000003, len=386] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261614400000,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507261615410003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261615410003,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202507261616420004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261616420004,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202507261617430005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261617430005,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202507261618440006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261618440006,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
data[type=4,serial=006EA1B2C3D4E5202507261619340007] 入待发送队列
push data[type=4, serial=MBCP00000008, len=419] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
运行状态数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261619340007,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/8
data[type=512,serial=006EA1B2C3D4E5202507261619450008] 入待发送队列
push data[type=512, serial=MBCP00000009, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261619450008,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/9
data[type=512,serial=006EA1B2C3D4E5202507261620460009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261620460009,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/10
data[type=512,serial=006EA1B2C3D4E5202507261621470010] 入待发送队列
push data[type=512, serial=MBCP00000011, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261621470010,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/11
data[type=512,serial=006EA1B2C3D4E5202507261622480011] 入待发送队列
push data[type=512, serial=MBCP00000012, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261622480011,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/12
data[type=512,serial=006EA1B2C3D4E5202507261623490012] 入待发送队列
push data[type=512, serial=MBCP00000013, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507261623490012,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
