云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507111402440000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_100, M_100, L_100
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507111402450001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507111402450002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507111402440000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507111402450002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507111402450001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507111403450003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507111403450003,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111854460000] 入待发送队列
Total consumption of ink on startup：0_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111855470001] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111856480002] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111857490003] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111858500004] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4503250500092202507111859340005] 入待发送队列
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111859510006] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111900520007] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111901530008] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111902540009] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111903550010] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111904560011] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111905570012] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111906580013] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4503250500092202507111908180014] 入待发送队列
data[type=4,serial=00F4503250500092202507111908210015] 入待发送队列
iot_status:-1
iot_status:-1
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=00F4203250100854202507111912010000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4203250100854202507111913020001] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
Total consumption of ink on startup：6_[W], [PRINT]S_0, M_0, L_0, [FLASH]S_0, M_0, L_0
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4203250100854202507111914030002] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4203250100854202507111915040003] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4203250100854202507111916050004] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
data[type=4,serial=00F4203250100854202507111916490005] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4203250100854202507111917060006] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4203250100854202507111918070007] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=00F4203250100854202507111919080008] 入待发送队列
HTTP丢包率：0/0
data[type=512,serial=00F4203250100854202507112153530009] 入待发送队列
data[type=4,serial=00F4203250100854202507112153530010] 入待发送队列
