云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507241034430000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
Total consumption of ink on startup：4_[Lc], [PRINT]S_0, M_0, L_0, [FLASH]S_240, M_240, L_240
Total consumption of ink on startup：5_[Lm], [PRINT]S_0, M_0, L_0, [FLASH]S_240, M_240, L_240
Total consumption of ink on startup：10_[-W], [PRINT]S_0, M_0, L_0, [FLASH]S_480, M_480, L_480
Total consumption of ink on startup：11_[-V], [PRINT]S_0, M_0, L_0, [FLASH]S_480, M_480, L_480
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507241034430001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507241034430002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241034430000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
iot_status:0
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241034430002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241034430001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507241035440003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241035440003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202507241036450004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241036450004,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202507241037460005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241037460005,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：4_[Lc], [PRINT]S_0, M_0, L_0, [FLASH]S_80, M_80, L_80
Total consumption of ink on startup：5_[Lm], [PRINT]S_0, M_0, L_0, [FLASH]S_80, M_80, L_80
Total consumption of ink on startup：10_[-W], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
Total consumption of ink on startup：11_[-V], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507241653390000] 入待发送队列
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507241653390001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507241653390002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241653390000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241653390002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241653390001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507241654400003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241654400003,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202507241655410004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241655410004,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202507241656420005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241656420005,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202507241657430006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507241657430006,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/7
data[type=512,serial=006EA1B2C3D4E5202507241658440007] 入待发送队列
push data[type=512, serial=MBCP00000008, len=396] via MB SUCCESSED, 剩余:0
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
