云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
CLOUD_PLATFORM线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250501657202507181009340000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_262144, M_262144, L_262144
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_262144, M_262144, L_262144
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_262144, M_262144, L_262144
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_262144, M_262144, L_262144
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
iot_status:-1
iot_status:-1
server-addr:http://hs.hosonsoft.com/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=0014203250501657202507181019260000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_5629499532902380, M_5629499532902380, L_5629499532902380
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_5629499532902380, M_5629499532902380, L_5629499532902380
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_5629499532902380, M_5629499532902380, L_5629499532902380
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_5629499532902380, M_5629499532902380, L_5629499532902380
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=0014203250501657202507181020270001] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=0014203250501657202507181021280002] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=0014203250501657202507181021490004] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
HTTP丢包率：0/0
data[type=512,serial=0014203250501657202507181022290005] 入待发送队列
iot_status:-1
iot_status:-1
iot_status:-1
iot_status:-1
Total consumption of ink on startup：0_[K], [PRINT]S_524288, M_524288, L_524288, [FLASH]S_5629499534213100, M_5629499534213100, L_5629499534213100
Total consumption of ink on startup：1_[C], [PRINT]S_524288, M_524288, L_524288, [FLASH]S_5629499534213100, M_5629499534213100, L_5629499534213100
Total consumption of ink on startup：2_[M], [PRINT]S_524288, M_524288, L_524288, [FLASH]S_5629499534213100, M_5629499534213100, L_5629499534213100
Total consumption of ink on startup：3_[Y], [PRINT]S_524288, M_524288, L_524288, [FLASH]S_5629499534213100, M_5629499534213100, L_5629499534213100
Total consumption of ink on startup：0_[K], [PRINT]S_1125899906842620, M_1125899906842620, L_1125899906842620, [FLASH]S_6755399440531432, M_6755399440531432, L_6755399440531432
Total consumption of ink on startup：1_[C], [PRINT]S_1125899906842620, M_1125899906842620, L_1125899906842620, [FLASH]S_6755399440531432, M_6755399440531432, L_6755399440531432
Total consumption of ink on startup：2_[M], [PRINT]S_1125899906842620, M_1125899906842620, L_1125899906842620, [FLASH]S_6755399440531432, M_6755399440531432, L_6755399440531432
Total consumption of ink on startup：3_[Y], [PRINT]S_1125899906842620, M_1125899906842620, L_1125899906842620, [FLASH]S_6755399440531432, M_6755399440531432, L_6755399440531432
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=2,serial=0014203250501657202507181023050006] 入待发送队列
墨点大小,SMB:1000000000.000000-1000000000.000000-1000000000.000000
data[type=1,serial=0014203250501657202507181023050007] 入待发送队列
iot_status:-1
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507181349170000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_1440, M_1440, L_1440
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_130, M_130, L_130
Total consumption of ink on startup：5_[LC], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：6_[LM], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：7_[LK], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
Total consumption of ink on startup：8_[LLk], [PRINT]S_0, M_0, L_0, [FLASH]S_40, M_40, L_40
iot_ccid:CCID-123, imei:IMEI-123
data[type=256,serial=006EA1B2C3D4E5202507181349170001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507181349170002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181349170000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181349170002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181349170001,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507181350180003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181350180003,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202507181351190004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181351190004,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507181927140000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_160, M_160, L_160
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507181927140001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507181927140002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181927140000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181927140002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181927140001,提交成功(0)
iot_status:0
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507181939580000] 入待发送队列
data[type=256,serial=006EA1B2C3D4E5202507181939580001] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_520, M_520, L_520
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_360, M_360, L_360
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_360, M_360, L_360
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_400, M_400, L_400
iot_ccid:CCID-123, imei:IMEI-123
push data[type=256, serial=MBCP00000001, len=468] via MB SUCCESSED, 剩余:1
data[type=128,serial=006EA1B2C3D4E5202507181939580002] 入待发送队列
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181939580001,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181939580002,提交成功(0)
push data[type=512, serial=MBCP00000003, len=386] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181939580000,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507181940590003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181940590003,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/4
data[type=512,serial=006EA1B2C3D4E5202507181942000004] 入待发送队列
push data[type=512, serial=MBCP00000005, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181942000004,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202507181943010005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181943010005,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1480, M_1480, L_1480
Total consumption of ink on startup：1_[C], [PRINT]S_800, M_800, L_800, [FLASH]S_840, M_840, L_840
Total consumption of ink on startup：2_[M], [PRINT]S_800, M_800, L_800, [FLASH]S_840, M_840, L_840
Total consumption of ink on startup：3_[Y], [PRINT]S_1000, M_1000, L_1000, [FLASH]S_1000, M_1000, L_1000
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/6
data[type=512,serial=006EA1B2C3D4E5202507181944020006] 入待发送队列
push data[type=512, serial=MBCP00000007, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181944020006,提交成功(0)
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1640, M_1640, L_1640
Total consumption of ink on startup：1_[C], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_920, M_920, L_920
Total consumption of ink on startup：2_[M], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_920, M_920, L_920
Total consumption of ink on startup：3_[Y], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1100, M_1100, L_1100
iot_status:0
RECV data from IOT, len=532
墨点大小,SMB:3.000000-5.000000-8.500000
data[type=2,serial=006EA1B2C3D4E5202507181944150007] 入待发送队列
墨点大小,SMB:3.000000-5.000000-8.500000
data[type=1,serial=006EA1B2C3D4E5202507181944150008] 入待发送队列
push data[type=1, serial=MBCP00000008, len=959] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181944150008,提交成功(0)
push data[type=2, serial=MBCP00000009, len=959] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181944150007,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/9
data[type=512,serial=006EA1B2C3D4E5202507181945030009] 入待发送队列
push data[type=512, serial=MBCP00000010, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181945030009,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507181953460000] 入待发送队列
data[type=256,serial=006EA1B2C3D4E5202507181953460001] 入待发送队列
push data[type=256, serial=MBCP00000001, len=468] via MB SUCCESSED, 剩余:1
Total consumption of ink on startup：0_[K], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1880, M_1880, L_1880
Total consumption of ink on startup：1_[C], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：2_[M], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1080, M_1080, L_1080
Total consumption of ink on startup：3_[Y], [PRINT]S_2000, M_2000, L_2000, [FLASH]S_1280, M_1280, L_1280
iot_ccid:CCID-123, imei:IMEI-123
data[type=128,serial=006EA1B2C3D4E5202507181953460002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181953460001,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181953460002,提交成功(0)
push data[type=512, serial=MBCP00000003, len=386] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181953460000,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507181954470003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507181954470003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507182006030000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_0, M_0, L_0, [FLASH]S_380, M_380, L_380
Total consumption of ink on startup：1_[C], [PRINT]S_0, M_0, L_0, [FLASH]S_60, M_60, L_60
Total consumption of ink on startup：2_[M], [PRINT]S_0, M_0, L_0, [FLASH]S_60, M_60, L_60
Total consumption of ink on startup：3_[Y], [PRINT]S_0, M_0, L_0, [FLASH]S_60, M_60, L_60
Total consumption of ink on startup：12_[-W], [PRINT]S_0, M_0, L_0, [FLASH]S_200, M_200, L_200
Total consumption of ink on startup：13_[-V], [PRINT]S_0, M_0, L_0, [FLASH]S_120, M_120, L_120
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507182006030001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507182006030002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182006030000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182006030002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182006030001,提交成功(0)
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_1800, M_1800, L_1800, [FLASH]S_1460, M_1460, L_1460
Total consumption of ink on startup：1_[C], [PRINT]S_200, M_200, L_200, [FLASH]S_180, M_180, L_180
Total consumption of ink on startup：2_[M], [PRINT]S_200, M_200, L_200, [FLASH]S_180, M_180, L_180
Total consumption of ink on startup：3_[Y], [PRINT]S_200, M_200, L_200, [FLASH]S_180, M_180, L_180
Total consumption of ink on startup：12_[-W], [PRINT]S_800, M_800, L_800, [FLASH]S_680, M_680, L_680
Total consumption of ink on startup：13_[-V], [PRINT]S_400, M_400, L_400, [FLASH]S_360, M_360, L_360
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507182007040003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182007040003,提交成功(0)
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
Total consumption of ink on startup：0_[K], [PRINT]S_3600, M_3600, L_3600, [FLASH]S_1640, M_1640, L_1640
Total consumption of ink on startup：1_[C], [PRINT]S_400, M_400, L_400, [FLASH]S_200, M_200, L_200
Total consumption of ink on startup：2_[M], [PRINT]S_400, M_400, L_400, [FLASH]S_200, M_200, L_200
Total consumption of ink on startup：3_[Y], [PRINT]S_400, M_400, L_400, [FLASH]S_200, M_200, L_200
Total consumption of ink on startup：12_[-W], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_760, M_760, L_760
Total consumption of ink on startup：13_[-V], [PRINT]S_800, M_800, L_800, [FLASH]S_400, M_400, L_400
iot_status:0
RECV data from IOT, len=532
墨点大小,SMB:3.000000-5.000000-8.500000
data[type=2,serial=006EA1B2C3D4E5202507182007290004] 入待发送队列
push data[type=2, serial=MBCP00000005, len=1035] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
作业数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182007290004,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
HTTP丢包率：0/5
data[type=512,serial=006EA1B2C3D4E5202507182008050005] 入待发送队列
push data[type=512, serial=MBCP00000006, len=396] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182008050005,提交成功(0)
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507182014340000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_7200, M_7200, L_7200, [FLASH]S_3980, M_3980, L_3980
Total consumption of ink on startup：1_[C], [PRINT]S_800, M_800, L_800, [FLASH]S_460, M_460, L_460
Total consumption of ink on startup：2_[M], [PRINT]S_800, M_800, L_800, [FLASH]S_460, M_460, L_460
Total consumption of ink on startup：3_[Y], [PRINT]S_800, M_800, L_800, [FLASH]S_460, M_460, L_460
Total consumption of ink on startup：12_[-W], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_1800, M_1800, L_1800
Total consumption of ink on startup：13_[-V], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_920, M_920, L_920
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507182014340001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507182014340002] 入待发送队列
iot_status:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182014340000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182014340002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182014340001,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507182015350003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182015350003,提交成功(0)
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
云模块版本:2.1.0.0
DATA SUBCRIBER:[CLOUD_PLATFORM,]
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
server-addr:http://pt.hosonsoft.com:5000/footstone-server/api/kdata
HTTP丢包率：0/0
data[type=512,serial=006EA1B2C3D4E5202507182017320000] 入待发送队列
Total consumption of ink on startup：0_[K], [PRINT]S_7200, M_7200, L_7200, [FLASH]S_4520, M_4520, L_4520
Total consumption of ink on startup：1_[C], [PRINT]S_800, M_800, L_800, [FLASH]S_520, M_520, L_520
Total consumption of ink on startup：2_[M], [PRINT]S_800, M_800, L_800, [FLASH]S_520, M_520, L_520
Total consumption of ink on startup：3_[Y], [PRINT]S_800, M_800, L_800, [FLASH]S_520, M_520, L_520
Total consumption of ink on startup：12_[-W], [PRINT]S_3200, M_3200, L_3200, [FLASH]S_2040, M_2040, L_2040
Total consumption of ink on startup：13_[-V], [PRINT]S_1600, M_1600, L_1600, [FLASH]S_1040, M_1040, L_1040
iot_ccid:CCID-123, imei:IMEI-123
push data[type=512, serial=MBCP00000001, len=386] via MB SUCCESSED, 剩余:0
data[type=256,serial=006EA1B2C3D4E5202507182017320001] 入待发送队列
data[type=128,serial=006EA1B2C3D4E5202507182017320002] 入待发送队列
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182017320000,提交成功(0)
push data[type=128, serial=MBCP00000002, len=404] via MB SUCCESSED, 剩余:1
RECV data from IOT, len=532
iot基站数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182017320002,提交成功(0)
push data[type=256, serial=MBCP00000003, len=468] via MB SUCCESSED, 剩余:0
iot_status:0
RECV data from IOT, len=532
iot-sim数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182017320001,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
HTTP丢包率：0/3
data[type=512,serial=006EA1B2C3D4E5202507182018330003] 入待发送队列
push data[type=512, serial=MBCP00000004, len=396] via MB SUCCESSED, 剩余:0
RECV data from IOT, len=532
心跳数据(serial:0000000000, 流水:006EA1B2C3D4E5202507182018330003,提交成功(0)
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
iot_status:0
RECV data from IOT, len=532
RECV data from IOT, len=532
RECV data from IOT, len=532
CLOUD_PLATFORM线程退出
CloudServiceCore线程退出
iot_status:0
